Flood Building Impact Function
==============================

Overview
--------

**Rating**: 0

**Limitation**: Lorem ipsum limitation

**Title**: Be flooded

**Unique Identifier**: Flood Building Impact Function

**Permissible Hazard Input**: A raster layer where each cell represents flood depth, or a vector polygon layer where each polygon represents an inundated area. The following attributes are recognised (in order): Flooded (True or False), FLOODPRONE (Yes or No) and Affected (True or False).

**Author**: Ole Nielsen, Kristy van Putten

**Actions**: Provide details about where critical response areas are

**Synopsis**: To assess the impacts of inundation on building footprints originating from OpenStreetMap (OSM).

**Citations**: 

* Hutchings, Field & Parks. Assessment of Flood impacts on buildings. Impact. Vol 66(2). 2012


**Permissible Exposure Input**: vector polygon layer extracted from OSM where each polygon represents the footprint of a building.

Details
-------

This is an area for free form text where adetailed description of the methodology used is given.