Stream Power Index
ta_hydrology
ParameterRaster|SLOPE|Slope|False
ParameterRaster|AREA|Catchment Area|False
ParameterSelection|CONV|Area Conversion|[0] no conversion (areas already given as specific catchment area);[1] 1 / cell size (pseudo specific catchment area)
OutputRaster|SPI|Stream Power Index
