# GDAL: Export Raster

O.Conrad (c) 2007
The "GDAL Raster Export" module exports one or more grids to various file formats using the "Geospatial Data Abstraction Library" (GDAL) by Frank Warmerdam. For more information have a look at the GDAL homepage:
http://www.gdal.org
GDAL Version:1.8.1
Following raster formats are currently supported:

ID | Name
--- | ---
VRT | Virtual Raster
GTiff | GeoTIFF
NITF | National Imagery Transmission Format
HFA | Erdas Imagine Images (.img)
ELAS | ELAS
MEM | In Memory Raster
BMP | MS Windows Device Independent Bitmap
PCIDSK | PCIDSK Database File
ILWIS | ILWIS Raster Map
SGI | SGI Image File Format 1.0
Leveller | Leveller heightfield
Terragen | Terragen heightfield
HDF4Image | HDF4 Dataset
ERS | ERMapper .ers Labelled
RMF | Raster Matrix Format
RST | Idrisi Raster A.1
INGR | Intergraph Raster
GSBG | Golden Software Binary Grid (.grd)
PNM | Portable Pixmap Format (netpbm)
ENVI | ENVI .hdr Labelled
EHdr | ESRI .hdr Labelled
PAux | PCI .aux Labelled
MFF | Vexcel MFF Raster
MFF2 | Vexcel MFF2 (HKV) Raster
BT | VTP .bt (Binary Terrain) 1.3 Format
IDA | Image Data and Analysis
GTX | NOAA Vertical Datum .GTX
NTv2 | NTv2 Datum Grid Shift
ADRG | ARC Digitized Raster Graphics
SAGA | SAGA GIS Binary Grid (.sdat)

## Parameters

Grid system
Grid system
  Grid system
Grid(s)
Input Grid list
File
File path
Format
Choice
  Available choices: Virtual Raster, GeoTIFF, National Imagery Transmission Format, Erdas Imagine Images (.img), ELAS, In Memory Raster, MS Windows Device Independent Bitmap, PCIDSK Database File, ILWIS Raster Map, SGI Image File Format 1.0, Leveller heightfield, Terragen heightfield, HDF4 Dataset, ERMapper .ers Labelled, Raster Matrix Format, Idrisi Raster A.1, Intergraph Raster, Golden Software Binary Grid (.grd), Portable Pixmap Format (netpbm), ENVI .hdr Labelled, ESRI .hdr Labelled, PCI .aux Labelled, Vexcel MFF Raster, Vexcel MFF2 (HKV) Raster, VTP .bt (Binary Terrain) 1.3 Format, Image Data and Analysis, NOAA Vertical Datum .GTX, NTv2 Datum Grid Shift, ARC Digitized Raster Graphics, SAGA GIS Binary Grid (.sdat)
Data Type
Choice
  Available choices: match input data, 8 bit unsigned integer, 16 bit unsigned integer, 16 bit signed integer, 32 bit unsigned integer, 32 bit signed integer, 32 bit floating point, 64 bit floating point