# IHACRES Calibration (2)

copyrights (c) 2008 Stefan Liersch
Calibration Tool for the Model IHACRES
Reference:
Jakeman, A.J. / Hornberger, G.M. (1993).
How Much Complexity Is Warranted in a Rainfall-Runoff Model?
Water Resources Research, (29), NO. 8 (2637-2649)
Croke, B. F. W., W. S. Merritt, et al. (2004).
A dynamic model for predicting hydrologic response to land cover changes in gauged and ungauged catchments.
Journal Of Hydrology 291(1-2): 115-131.

## Parameters

Table
Output Data Object
Table
Input Table
Date Column
Table field
  Select the column containing the Date
Streamflow Column
Table field
  Select the Column containing Discharge Values
Precipitation Column
Table field
  Select the Column containing precipitation Values
Temperature Column
Table field
  Select the Column containing Temperature Values
Subbasin Inflow
Table field
  Select the column containing inflow data to the subbasin
Is the subbasin upstream (no external inflow)
Boolean
  If checked, it means there is no external inflow to the subbasin
Using temperature data?
Boolean
  If checked, then temperature data are used.
Number of Simulations
Integer
  Number of Simulations for Calibration
  Minimum: 1.0; Maximum: 10000000.0
Area of the Watershed in [km2]
Floating point
  Area of the Watershed in [km2] used for unit conversion
  Minimum: 1e-05
Storage Configuration
Node
Storage
Choice
  Available choices: Single Storage, Two Parallel Storages, Two Storages in Series
IHACRES Version
Node
IHACRES Version
Choice
  Available choices: Jakeman & Hornberger (1993), Croke et al. (2005)
Snow Module on/off
Boolean
  If checked the snow module is active
Table
Output Data Object
Table
Output Data Object