# Fuzzify

Victor Olaya (c) 2004
Translates grid values into fuzzy set membership as preparation for fuzzy logic analysis.

## Parameters

Grid system
Grid system
  Grid system
Grid
Input Grid
Fuzzified Grid
Output Grid
Control Points
Node
A
Floating point
  Values lower than A will be set to 0.
B
Floating point
  Values between A and B increase from 0 to 1, values between B and C will be set to 1.
C
Floating point
  Values between B and C will be set to 1, values between C and D decrease from 1 to 0.
D
Floating point
  Values greater than D will be set to 0.
Membership Function Type
Choice
  Available choices: linear, sigmoidal, j-shaped
Adjust to Grid
Boolean
  Automatically adjust control points to grid's data range