# Overland Flow - Kinematic Wave D8

O. Conrad (c) 2003
Overland Flow - Kinematic Wave D8
Reference:
Johnson, D.L., Miller, A.C. (1997): A spatially distributed hydrological model utilizing raster data structures, Computers & Geosciences, Vol.23, No.3, pp.267-272

## Parameters

Grid system
Grid system
  Grid system
Elevation
Input Grid
Runoff
Output Grid
Gauges
Input Shapes
Flow at Gauges
Output Table
Simulation Time [h]
Floating point
Simulation Time Step [h]
Floating point
Manning's Roughness
Floating point
Newton-Raphson
Node
Max. Iterations
Integer
  Minimum: 1.0
Epsilon
Floating point
Precipitation
Choice
  Kind of initializing Precipitation Event
  Available choices: Homogenous, Above Elevation, Left Half
Threshold Elevation
Floating point