# RGB Composite

(c) 2002 by O.Conrad
Create red-green-blue overlays of grids.

## Parameters

Grid system
Grid system
  Grid system
Red
Input Grid
Value Preparation
Choice
  Available choices: 0 - 255, Rescale to 0 - 255, User defined rescale, Percentiles, Percentage of standard deviation
Rescale Range
Value range
  Minimum: 1.40053539606e-316; Maximum: 1.40047927021e-316
Percentiles
Value range
  Minimum: 1.40065318131e-316; Maximum: 1.40060733202e-316
Percentage of standard deviation
Floating point
Green
Input Grid
Value Preparation
Choice
  Available choices: 0 - 255, Rescale to 0 - 255, User defined rescale, Percentiles, Percentage of standard deviation
Rescale Range
Value range
  Minimum: 1.40095594474e-316; Maximum: 1.40090139989e-316
Percentiles
Value range
  Minimum: 1.40106503444e-316; Maximum: 1.40102076615e-316
Percentage of standard deviation
Floating point
Blue
Input Grid
Value Preparation
Choice
  Available choices: 0 - 255, Rescale to 0 - 255, User defined rescale, Percentiles, Percentage of standard deviation
Rescale Range
Value range
  Minimum: 1.40136147382e-316; Maximum: 1.40118914373e-316
Percentiles
Value range
  Maximum: 1.40143340978e-316
Percentage of standard deviation
Floating point
Transparency
Input Grid
Value Preparation
Choice
  Available choices: 0 - 255, Rescale to 0 - 255, User defined rescale, Percentiles, Percentage of standard deviation
Rescale Range
Value range
  Minimum: 1.40177569846e-316; Maximum: 1.40173617321e-316
Percentiles
Value range
  Minimum: 1.40189269321e-316; Maximum: 1.40184684391e-316
Percentage of standard deviation
Floating point
Composite
Output Grid