Additional data

This step is optional

Description This step allow user to integrate additional data to selected land cover classes.

Parameters
Input layer can be vector or raster.
If input layer is vector, user can specify a selection Expression (matching features are selected) and a Buffer (applied to selected features to modelize physical footprint). If expression is empty, all features are selected.
Choose a unique Identifier for current selection.
Set Fragmentation status according to data nature (roads are fragmentation data, green infrastructures are not).
Press Save selection to save current parameters (selections are then processed all at once) and rank resulting selection (new line in table) according to its priority.

Results
Press Integrate additional data to process data selection and integration.
Each selection is processed (clip, selection, buffer) and resulting layer (with identifier name) is stored in temporary directory.
Selections are ranked (higher priority selection will erase lower priority selection) with interface arrows and merged with landuse layer (step 2 output). Resulting layer is loaded in QGIS.