[general]
name=Geomaticape Tools
description=Landsat, Sentinel-2 and CBERS-04A preprocessing for professional GIS analysis
version=1.3
qgisMinimumVersion=3.22
author=Geomatica Ambiental
email=nino@geomatica.pe
authorUrl=https://www.geomatica.pe/

about=GeomaticaPE is a QGIS plugin developed by Geomatica Ambiental to automate the preprocessing of multispectral satellite imagery. It is designed for GIS professionals, researchers, and technicians who require efficient, reproducible workflows with analysis-ready outputs.

    Supported sensors:
    - Landsat 4/5 TM, 7 ETM+, 8/9 OLI-TIRS — Collection 2 Level 2
    - Sentinel-2 MSI — Level-1C and Level-2A
    - CBERS-04A WPM — Pansharpening at 2-meter resolution

    Key features:
    - Radiometric correction: applies official scale factors to obtain true surface reflectance
    - Land Surface Temperature: converts Landsat thermal band to degrees Celsius (°C)
    - Brovey Pansharpening: panchromatic fusion of CBERS-04A imagery at 2m with AOI clipping
    - Multiband output: generates GeoTIFF with internal band names automatically assigned
    - Automatic resampling: harmonizes spatial resolutions (10m, 20m, 60m) into a single image

    All tools are fully integrated into the QGIS Processing Panel, featuring a graphical interface, contextual help, and automatic cleanup of temporary files.

    Developed and maintained by:
    Geomatica Ambiental — www.geomatica.pe

icon=Icons/logo_geomatica.png

tracker=https://www.geomatica.pe/
repository=https://www.geomatica.pe/
homepage=https://www.geomatica.pe/
category=Raster
tags=landsat, sentinel, cbers, reflectance, pansharpening, remote sensing, scale factor, land surface temperature, raster, radiometric correction
hasProcessingProvider=yes
server=False
experimental=False
deprecated=False

changelog=1.3
    - New: CBERS-04A Brovey Pansharpening at 2m with vector AOI clipping
    1.2
    - Scale factor for Sentinel-2 L2A (10m) with automatic resampling of 20m and 60m bands
    - Scale factor for Sentinel-2 L1A
    - Scale factor for Landsat Collection 2 L2 (Surface Reflectance + Land Surface Temperature °C)
    - Support for Landsat 4/5 TM, 7 ETM+, 8/9 OLI/TIRS
    - Internal band names automatically assigned to output rasters