# Code Architecture

This chapter describes the internal architecture of OMRAT, including the module structure, class hierarchy, and data flow between components.

## Directory Structure

    OMRAT/
    ├── omrat.py                    # Main plugin class (entry point, slim facade)
    ├── omrat_widget.py             # Main UI dock widget
    ├── __init__.py                 # Plugin initialisation (classFactory)
    │
    ├── compute/                    # Risk calculation engine
    │   ├── basic_equations.py      # Core mathematical formulas
    │   ├── run_calculations.py     # Calculation orchestration
    │   ├── calculation_task.py     # QgsTask wrapper for background exec
    │   ├── drifting_model.py       # Drifting cascade (mixin onto Calculation)
    │   ├── database.py             # PostgreSQL/PostGIS connector
    │   └── iwrap_convertion.py     # IWRAP XML import/export
    │
    ├── geometries/                 # Spatial geometry operations
    │   ├── handle_qgis_iface.py    # Route digitisation & layer mgmt
    │   ├── route.py                # Route processing utilities
    │   ├── drift_corridor_v2.py    # Drift corridor API (re-exports)
    │   ├── drift_corridor_task_v2.py  # Background corridor generation
    │   ├── get_drifting_overlap.py # Overlap dialog facade + visualizer class
    │   ├── drift_overlap_geometry.py  # Pure geometry/distance helpers
    │   ├── drift_overlap_plot.py   # Bottom PDF panel matplotlib helper
    │   ├── drift_overlap_sidebar.py   # Sortable QTableWidget sidebar builder
    │   ├── calculate_probability_holes.py  # Monte Carlo integration
    │   ├── result_layers.py        # Result QGIS layer creation
    │   └── drift/                  # Refactored drift submodule
    │       ├── constants.py        # Direction constants (N,NE,E,...)
    │       ├── coordinates.py      # CRS transformations
    │       ├── distribution.py     # Width & projection distance
    │       ├── corridor.py         # Base surface & projected corridor
    │       ├── shadow.py           # Obstacle blocking zones
    │       ├── clipping.py         # Corridor clipping & anchor split
    │       ├── generator.py        # Main corridor generator (~800 lines)
    │       └── probability_integration.py  # Probability hole integration
    │
    ├── omrat_utils/                # Data management + UI mixins
    │   ├── handle_traffic.py       # Traffic table management
    │   ├── handle_object.py        # Depth & structure management
    │   ├── handle_ais.py           # AIS database integration
    │   ├── handle_distributions.py # Lateral distribution modelling
    │   ├── handle_settings.py      # Drift parameter configuration
    │   ├── handle_ship_cat.py      # Ship type classifications
    │   ├── causation_factors.py    # Causation factor management
    │   ├── gather_data.py          # Data serialisation/deserialisation
    │   ├── storage.py              # Project file I/O (.omrat JSON)
    │   ├── validate_data.py        # Pydantic validation schemas
    │   ├── repair_time.py          # Repair time distribution
    │   ├── units.py                # Unit conversion utilities
    │   ├── iwrap_io_mixin.py       # OMRAT IWRAP import/export slots
    │   ├── compare_mixin.py        # Compare-Models tab logic
    │   ├── drift_analysis_mixin.py # Drift-corridor analysis runner + layers
    │   ├── run_history_mixin.py    # Auto-save flow + Previous-runs table
    │   └── accident_results_mixin.py  # TWAccidentResults + per-row View dispatcher
    │
    ├── ui/                         # User interface widgets
    │   ├── drift_settings_widget.py
    │   ├── traffic_data_widget.py
    │   ├── ship_categories_widget.py
    │   ├── ais_connection_widget.py
    │   ├── causation_factor_widget.py
    │   ├── result_widget.py
    │   └── show_geom_res.py
    │
    ├── helpers/                    # Helper utilities
    │   └── qt_conversions.py       # Qt5/Qt6 compatibility
    │
    ├── tests/                      # Test suite
    └── help/                       # Documentation (Sphinx)

## Data Flow

The following diagram shows how data flows through OMRAT from input to output:

The data flow can be summarised in five phases:

1. Input: Routes are digitised on the map, traffic data is entered or imported from AIS, obstacles are loaded from shapefiles or GEBCO.

2. Collection: `gather_data.py` aggregates all data into a single dictionary for calculation and persistence.

3. Transformation: Geometries are transformed from WGS84 to UTM for accurate distance-based calculations.

4. Calculation: Three parallel pipelines compute drifting risk, powered risk, and collision risk.

5. Output: Results are visualised as QGIS layers and stored in the project file.

## Key Classes

### OMRAT (omrat.py)

The main plugin class. It owns the manager components and orchestrates the plugin lifecycle, but most slot-handling logic now lives in focused mixins under `omrat_utils/`. The class declaration is:

    class OMRAT(
        IwrapIOMixin, CompareMixin, DriftAnalysisMixin, RunHistoryMixin,
        AccidentResultsMixin,
    ):
        ...

What `omrat.py` itself still owns:

- Initialisation: Creates instances of all manager classes (Traffic, OObject, DriftSettings, etc.)

- Signal management: Connects UI buttons to handler methods

- Calculation dispatch: Creates `CalculationTask` or `DriftCorridorTask` instances for background execution

- Menu/toolbar: Registers QGIS menu items and toolbar buttons

What the mixins own:

- `IwrapIOMixin` – IWRAP XML import / export menu actions

- `CompareMixin` – the Compare Models tab (snapshot pickers, diff tables, layer overlays)

- `DriftAnalysisMixin` – Run Drift Analysis slot, per-leg categorised polygon layers

- `RunHistoryMixin` – auto-save flow (`.omrat` snapshot, `.gpkg`, `.collision.json` and `.drifting.json` sidecars, `_results_<timestamp>.md`) plus the Previous runs table

- `AccidentResultsMixin` – the `TWAccidentResults` table with per-row View buttons that dispatch to the interactive visualiser of the selected previous run

`omrat.py` – OMRAT (main plugin entry point) | IwrapIOMixin, CompareMixin, DriftAnalysisMixin, RunHistoryMixin, AccidentResultsMixin

### OMRATMainWidget (omrat_widget.py)

The Qt dock widget that provides the user interface. It is built from `omrat_base.ui` (Qt Designer file) and contains:

- Route tab: Route table, digitisation buttons

- Traffic tab: Ship frequency/speed/dimension tables

- Depths tab: Depth polygon management, GEBCO download

- Objects tab: Structure polygon management

- Distributions tab: Lateral distribution configuration and plots

- Results tab: Calculation results display

- Drift Analysis tab: Corridor generation controls

### Calculation (compute/run_calculations.py)

The main calculation engine. Key responsibilities:

- `run_drifting_model(data)`: Computes drifting grounding/allision probabilities using Monte Carlo integration

- `run_ship_collision_model(data)`: Computes ship-ship collision frequencies

- `run_powered_grounding_model(data)`: Computes powered grounding

    (Category I and II) with depth-bin caching and per-bin progress updates

- `run_powered_allision_model(data)`: Computes powered allision

- `run_drift_visualization(data)`: Creates visual corridor layers

`compute/run_calculations.py:44` – Calculation (mixin-based facade) | Mixins: DriftingModelMixin, ShipCollisionModelMixin, PoweredModelMixin, DriftingReportMixin, VisualizationMixin

### DriftCorridorGenerator (geometries/drift/generator.py)

Orchestrates drift corridor generation for all legs and directions:

- `precollect_data()`: Gathers UI data in the main thread (required because Qt widgets are thread-unsafe)

- `generate_corridors()`: Generates corridors in a background thread

- `_create_single_corridor()`: Creates one corridor for one leg in one direction

`geometries/drift/generator.py:25` – DriftCorridorGenerator | `geometries/drift/generator.py:65` – precollect_data() | `geometries/drift/generator.py:360` – generate_corridors() | `geometries/drift/generator.py:516` – _create_single_corridor()

### HandleQGISIface (geometries/handle_qgis_iface.py)

Manages QGIS layer operations for route digitisation:

- Route creation via map click tool

- Segment data tracking (start/end points, directions, widths)

- Visual offset lines showing route width

- Geometry change detection for interactive editing

- Geometry edit persistence: map edits are synchronised back to

    `segment_data` (start/end points, directions, and line length), so save/export use the edited geometry

`geometries/handle_qgis_iface.py` – HandleQGISIface

## Data Structures

### Traffic Data

Traffic data is stored in a nested dictionary:

    traffic_data[segment_id][direction] = {
        'Frequency (ships/year)': [[int, ...], ...],   # [type][size]
        'Speed (knots)':          [[float, ...], ...],
        'Draught (meters)':       [[float, ...], ...],
        'Ship heights (meters)':  [[float, ...], ...],
        'Ship Beam (meters)':     [[float, ...], ...],
    }

Each value is a 2D array indexed by `[ship_type_index][ship_size_index]`.

### Segment Data

    segment_data[segment_id] = {
        'Start_Point': str,      # WKT point
        'End_Point': str,        # WKT point
        'Dirs': [str, str],      # Direction labels
        'Width': float,          # Lane width (m)
        'line_length': float,    # Segment length (m)
        'Route_Id': int,
        'Leg_name': str,
        'Segment_Id': int,
        # Distribution parameters:
        'mean1_1': float, 'std1_1': float, 'weight1_1': float,
        'mean1_2': float, 'std1_2': float, 'weight1_2': float,
        'mean1_3': float, 'std1_3': float, 'weight1_3': float,
        'u_min1': float, 'u_max1': float, 'u_p1': float,
        # ... same for direction 2 ...
    }

### Drift Values

    drift_values = {
        'drift_p': float,           # Blackout frequency
        'anchor_p': float,          # Anchor probability
        'anchor_d': float,          # Max anchorable depth (m)
        'speed': float,             # Drift speed (m/s)
        'rose': {                   # Wind rose probabilities
            '0': float,             # North
            '45': float,            # NorthWest
            '90': float,            # West
            '135': float,           # SouthWest
            '180': float,           # South
            '225': float,           # SouthEast
            '270': float,           # East
            '315': float,           # NorthEast
        },
        'repair': {
            'func': str,            # Custom function expression
            'std': float,           # Lognormal shape
            'loc': float,           # Location parameter
            'scale': float,         # Scale parameter
            'use_lognormal': bool,  # Use lognormal or custom
        }
    }

## Background Task Execution

OMRAT uses QGIS’s `QgsTask` system for long-running calculations. This keeps the UI responsive while computations run in background threads.

### CalculationTask

Wraps the full risk calculation pipeline:

1. `run_drifting_model()` – probability holes (60% of time)

2. `run_ship_collision_model()` – collision frequencies (fast)

3. `run_powered_grounding_model()` – powered grounding

4. `run_powered_allision_model()` – powered allision

Signals emitted: `progress_updated`, `calculation_finished`, `calculation_failed`.

`compute/calculation_task.py` – CalculationTask

### DriftCorridorTask

Wraps the drift corridor generation:

1. `precollect_data()` runs in the main thread (before task starts)

2. `generate_corridors()` runs in the background thread

3. Layer creation runs in the main thread (via `finished()` signal)

Signals emitted: `progress_updated`, `corridors_generated`, `generation_failed`.

`geometries/drift_corridor_task_v2.py` – DriftCorridorTask

## IWRAP Integration

OMRAT supports bidirectional conversion with IWRAP XML format:

Export (`write_iwrap_xml`):

1. Gather project data via `GatherData`

2. Build XML tree with waypoints, legs, traffic distributions, obstacles

3. Write formatted XML file

Import (`parse_iwrap_xml`):

1. Parse XML tree structure

2. Extract waypoints, legs, traffic, causation factors

3. Map to OMRAT’s internal data format

4. Validate with Pydantic schema

5. Populate UI via `GatherData.populate()`

The conversion handles differences in data model between IWRAP and OMRAT, including coordinate format, traffic representation, and distribution parameters.

`compute/iwrap_convertion.py` – IWRAP conversion module

## Project Persistence

Projects are saved as `.omrat` files (JSON format):

    {
      "project_name": "My Analysis",
      "pc": {"p_pc": 1.6e-4, "d_pc": 1.0},
      "drift": {
        "drift_p": 1, "anchor_p": 0.95, "anchor_d": 7,
        "speed": 1.944, "rose": {...}, "repair": {...}
      },
      "traffic_data": {...},
      "segment_data": {...},
      "depths": [[id, depth, wkt], ...],
      "objects": [[id, height, wkt], ...],
      "ship_categories": {...}
    }

The `validate_data.py` module defines a Pydantic schema (`RootModelSchema`) that validates the structure on save and load. Legacy format conversion is handled by `Storage._normalize_legacy_to_schema()`.

`omrat_utils/storage.py` – Storage | `omrat_utils/validate_data.py` – Validation schemas