<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.28.15-Firenze">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract></abstract>
  <links/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["WGS 72BE / UTM zone 17N",BASEGEOGCRS["WGS 72BE",DYNAMIC[FRAMEEPOCH[1972]],DATUM["WGS 72 Transit Broadcast Ephemeris",ELLIPSOID["WGS 72",6378135,298.26,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4324]],CONVERSION["UTM zone 17N",METHOD["Transverse Mercator",ID["EPSG",9807]],PARAMETER["Latitude of natural origin",0,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8801]],PARAMETER["Longitude of natural origin",-81,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8802]],PARAMETER["Scale factor at natural origin",0.9996,SCALEUNIT["unity",1],ID["EPSG",8805]],PARAMETER["False easting",500000,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",0,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["(E)",east,ORDER[1],LENGTHUNIT["metre",1]],AXIS["(N)",north,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Engineering survey, topographic mapping."],AREA["Between 84°W and 78°W, northern hemisphere between equator and 84°N, onshore and offshore."],BBOX[0,-84,84,-78]],ID["EPSG",32417]]</wkt>
      <proj4>+proj=utm +zone=17 +ellps=WGS72 +towgs84=0,0,1.9,0,0,0.814,-0.38 +units=m +no_defs</proj4>
      <srsid>2981</srsid>
      <srid>32417</srid>
      <authid>EPSG:32417</authid>
      <description>WGS 72BE / UTM zone 17N</description>
      <projectionacronym>utm</projectionacronym>
      <ellipsoidacronym>EPSG:7043</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent/>
</qgis>
