Plan riparian buffer zones. This version works only in Finland as it uses pre-modelled data sets for retention of suspended solids. The method accumulates RUSLE values by the massflux method and determines cost values for the retention of suspended solids from a water body.

### Input parameters

- Planning area Planning or cutting area as vector polygon format

- Retention of suspended solidThe minimum percentage of suspended solids that should be retained in a riparian zone

- Minimum widthMinimum width of riparian zone

- Average widthAverage width of riparian zone

### Outputs

- Riparian zoneProposed riparian zone based on accumulation of suspended solid

Algorithm author: Mikko Kesälä