[general]
name = Tower Spotter
qgisMinimumVersion = 3.0
version = 1.3.3
description = Generates tower polygons at each vertex of LineString layers or imported KML files.
 Automatically performs dynamic UTM reprojection for accurate meter-based radius calculations.
 Output can be exported as Google Earth compatible KML (WGS84).
 No external dependencies required.

about = Tower Spotter creates tower footprint polygons for towers in transmission line and infrastructure planning workflows. 
 Designed for engineering use cases requiring accurate tower spotting  from geographic CRS layers. 
 Supports customizable radius, polygon sides, and colors.

author = Vicky Sharma
email = vsharma@powergrid.in
repository = https://github.com/ineffablexd/tower_spotter
homepage = https://github.com/ineffablexd/tower_spotter
tracker = https://github.com/ineffablexd/tower_spotter/issues
license = GPL-2.0-or-later
icon = icon.png
tags = tower, transmission, powerline, engineering, infrastructure, polygon, utm, kml
experimental = False
deprecated = False
