<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.40.0-Bratislava">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract></abstract>
  <links/>
  <dates/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["ETRF2000-PL / CS92",BASEGEOGCRS["ETRF2000-PL",DATUM["ETRF2000 Poland",ELLIPSOID["GRS 1980",6378137,298.257222101,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",9702]],CONVERSION["Poland CS92",METHOD["Transverse Mercator",ID["EPSG",9807]],PARAMETER["Latitude of natural origin",0,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8801]],PARAMETER["Longitude of natural origin",19,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8802]],PARAMETER["Scale factor at natural origin",0.9993,SCALEUNIT["unity",1],ID["EPSG",8805]],PARAMETER["False easting",500000,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",-5300000,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["northing (x)",north,ORDER[1],LENGTHUNIT["metre",1]],AXIS["easting (y)",east,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Topographic mapping (medium and small scale)."],AREA["Poland - onshore and offshore."],BBOX[49,14.14,55.93,24.15]],ID["EPSG",2180]]</wkt>
      <proj4>+proj=tmerc +lat_0=0 +lon_0=19 +k=0.9993 +x_0=500000 +y_0=-5300000 +ellps=GRS80 +towgs84=0,0,0,0,0,0,0 +units=m +no_defs</proj4>
      <srsid>171</srsid>
      <srid>2180</srid>
      <authid>EPSG:2180</authid>
      <description>ETRF2000-PL / CS92</description>
      <projectionacronym>tmerc</projectionacronym>
      <ellipsoidacronym>EPSG:7019</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent/>
</qgis>
