# QGIS Radiation Toolbox Plugin Documentation

This plugin allows to easily load data from Safecast radiation monitoring devices (LOG file) like bGeigie Nano or CzechRad into QGIS version 3 as a new vector point layer. The data are loaded using predefined color style.

The user can, if necessary, easily select and remove unwanted parts of the measurement set and save the corrected set as a new LOG file for uploading to Safecast web map.

Basic and experimental support for viewing ERS 2.0 format (European Radiometric and Spectrometry format) and some types of PicoEnvirotec PEI files is also available.

- Introduction
- Installation
- User Manual
  - Load LOG file
  - Layer statistics
  - Layer graph
  - Add background map (Google, Bing, OpenStreetMap or offline)
  - Browse attribute data
  - Delete measured points
  - Save changes into new LOG file
  - How to show values of particular point using Identify Features tool
- About
  - Acknowledgement
  - License
  - Report bugs or enhancements
  - Known issues