# sec_interp.gui.ui.pages.drillhole_page module

UI page for drillhole data configuration.

class sec_interp.gui.ui.pages.drillhole_page.DrillholePage(parent=None)

  Bases: `BasePage`

  Configuration page for Drillhole data (Collar, Survey, Intervals).

  Initialize the page.

  Parameters:

    - title (str) – Title for the group box.

    - parent (QWidget) – Parent widget.

  dataChanged

    str = …, revision: int = …, arguments: Sequence = …) -> PYQT_SIGNAL

    types is normally a sequence of individual types. Each type is either a type object or a string that is the name of a C++ type. Alternatively each type could itself be a sequence of types each describing a different overloaded signal. name is the optional C++ name of the signal. If it is not specified then the name of the class attribute that is bound to the signal is used. revision is the optional revision of the signal that is exported to QML. If it is not specified then 0 is used. arguments is the optional sequence of the names of the signal’s arguments.

    Type:

      pyqtSignal(*types, name

  get_data() → dict

    Get drillhole configuration.

  is_complete() → bool

    Check if required fields are filled if layers are selected.