# sec_interp.gui.services.parallel_geology_service module

Parallel geology processing service.

This module implements parallel processing capabilities for geology services using QThread.

class sec_interp.gui.services.parallel_geology_service.GeologyProcessingThread(data: list[Any], processing_func: Callable[[Any], Any])

  Bases: `QThread`

  Thread for parallel geological data processing.

  Initialize processing thread.

  Parameters:

    - data – List of items to process

    - processing_func – Function to process each item

  progress_updated

    str = …, revision: int = …, arguments: Sequence = …) -> PYQT_SIGNAL

    types is normally a sequence of individual types. Each type is either a type object or a string that is the name of a C++ type. Alternatively each type could itself be a sequence of types each describing a different overloaded signal. name is the optional C++ name of the signal. If it is not specified then the name of the class attribute that is bound to the signal is used. revision is the optional revision of the signal that is exported to QML. If it is not specified then 0 is used. arguments is the optional sequence of the names of the signal’s arguments.

    Type:

      pyqtSignal(*types, name

  processing_finished

    str = …, revision: int = …, arguments: Sequence = …) -> PYQT_SIGNAL

    types is normally a sequence of individual types. Each type is either a type object or a string that is the name of a C++ type. Alternatively each type could itself be a sequence of types each describing a different overloaded signal. name is the optional C++ name of the signal. If it is not specified then the name of the class attribute that is bound to the signal is used. revision is the optional revision of the signal that is exported to QML. If it is not specified then 0 is used. arguments is the optional sequence of the names of the signal’s arguments.

    Type:

      pyqtSignal(*types, name

  error_occurred

    str = …, revision: int = …, arguments: Sequence = …) -> PYQT_SIGNAL

    types is normally a sequence of individual types. Each type is either a type object or a string that is the name of a C++ type. Alternatively each type could itself be a sequence of types each describing a different overloaded signal. name is the optional C++ name of the signal. If it is not specified then the name of the class attribute that is bound to the signal is used. revision is the optional revision of the signal that is exported to QML. If it is not specified then 0 is used. arguments is the optional sequence of the names of the signal’s arguments.

    Type:

      pyqtSignal(*types, name

  canceled

    str = …, revision: int = …, arguments: Sequence = …) -> PYQT_SIGNAL

    types is normally a sequence of individual types. Each type is either a type object or a string that is the name of a C++ type. Alternatively each type could itself be a sequence of types each describing a different overloaded signal. name is the optional C++ name of the signal. If it is not specified then the name of the class attribute that is bound to the signal is used. revision is the optional revision of the signal that is exported to QML. If it is not specified then 0 is used. arguments is the optional sequence of the names of the signal’s arguments.

    Type:

      pyqtSignal(*types, name

  __init__(data: list[Any], processing_func: Callable[[Any], Any])

    Initialize processing thread.

    Parameters:

      - data – List of items to process

      - processing_func – Function to process each item

  cancel()

    Request thread cancellation.

  is_canceled() → bool

    Check if cancellation was requested.

  run()

    Execute processing in separate thread.

class sec_interp.gui.services.parallel_geology_service.ParallelGeologyService

  Bases: `QObject`

  Service with parallel processing using QThreads.

  all_finished

    str = …, revision: int = …, arguments: Sequence = …) -> PYQT_SIGNAL

    types is normally a sequence of individual types. Each type is either a type object or a string that is the name of a C++ type. Alternatively each type could itself be a sequence of types each describing a different overloaded signal. name is the optional C++ name of the signal. If it is not specified then the name of the class attribute that is bound to the signal is used. revision is the optional revision of the signal that is exported to QML. If it is not specified then 0 is used. arguments is the optional sequence of the names of the signal’s arguments.

    Type:

      pyqtSignal(*types, name

  batch_progress

    str = …, revision: int = …, arguments: Sequence = …) -> PYQT_SIGNAL

    types is normally a sequence of individual types. Each type is either a type object or a string that is the name of a C++ type. Alternatively each type could itself be a sequence of types each describing a different overloaded signal. name is the optional C++ name of the signal. If it is not specified then the name of the class attribute that is bound to the signal is used. revision is the optional revision of the signal that is exported to QML. If it is not specified then 0 is used. arguments is the optional sequence of the names of the signal’s arguments.

    Type:

      pyqtSignal(*types, name

  error_occurred

    str = …, revision: int = …, arguments: Sequence = …) -> PYQT_SIGNAL

    types is normally a sequence of individual types. Each type is either a type object or a string that is the name of a C++ type. Alternatively each type could itself be a sequence of types each describing a different overloaded signal. name is the optional C++ name of the signal. If it is not specified then the name of the class attribute that is bound to the signal is used. revision is the optional revision of the signal that is exported to QML. If it is not specified then 0 is used. arguments is the optional sequence of the names of the signal’s arguments.

    Type:

      pyqtSignal(*types, name

  processing_canceled

    str = …, revision: int = …, arguments: Sequence = …) -> PYQT_SIGNAL

    types is normally a sequence of individual types. Each type is either a type object or a string that is the name of a C++ type. Alternatively each type could itself be a sequence of types each describing a different overloaded signal. name is the optional C++ name of the signal. If it is not specified then the name of the class attribute that is bound to the signal is used. revision is the optional revision of the signal that is exported to QML. If it is not specified then 0 is used. arguments is the optional sequence of the names of the signal’s arguments.

    Type:

      pyqtSignal(*types, name

  process_profiles_parallel(profiles: list[Any], processing_func: Callable[[Any], Any] | None = None)

    Process multiple profiles in parallel using threads asynchronously.

    Parameters:

      - profiles – List of profiles to process

      - processing_func – Optional custom processing function. If None, uses internal _process_profile_chunk.

  cancel_processing()

    Cancel all active processing threads.