LS Factor
ta_hydrology
ParameterRaster|SLOPE|Slope|False
ParameterRaster|AREA|Catchment Area|False
ParameterSelection|CONV|Area to Length Conversion|[0] no conversion (areas already given as specific catchment area);[1] 1 / cell size (specific catchment area);[2] square root (catchment length)
ParameterSelection|METHOD|Method (LS)|[0] Moore et al. 1991;[1] Desmet & Govers 1996;[2] Boehner & Selige 2006
ParameterNumber|EROSIVITY|Rill/Interrill Erosivity|None|None|0.0
ParameterSelection|STABILITY|Stability|[0] stable;[1] instable (thawing)
OutputRaster|LS|LS Factor
