TOPMODEL
sim_hydrology
ParameterRaster|ATANB|Topographic Wetness Index|False
ParameterTable|WEATHER|Weather Records|False
ParameterTableField|RECORD_P|Precipitation [m / dt]|WEATHER
ParameterTableField|RECORD_ET|Evapotranspiration [m / dt]|WEATHER
ParameterTableField|RECORD_DATE|Date/Time|WEATHER
ParameterNumber|DTIME|Time Step [h]|None|None|1.0
ParameterNumber|NCLASSES|Number of Classes|None|None|30
ParameterNumber|P_QS0|Initial subsurface flow per unit area [m/h]|None|None|3.28e-05
ParameterNumber|P_LNTE|Areal average of ln(T0) = ln(Te) [ln(m^2/h)]|None|None|5.0
ParameterNumber|P_MODEL|Model parameter [m]|None|None|0.032
ParameterNumber|P_SR0|Initial root zone storage deficit [m]|None|None|0.002
ParameterNumber|P_SRZMAX|Maximum root zone storage deficit [m]|None|None|0.05
ParameterNumber|P_SUZ_TD|Unsaturated zone time delay per unit storage deficit [h]|None|None|50.0
ParameterNumber|P_VCH|Main channel routing velocity [m/h]|None|None|3600.0
ParameterNumber|P_VR|Internal subcatchment routing velocity [m/h]|None|None|3600.0
ParameterNumber|P_K0|Surface hydraulic conductivity [m/h]|None|None|1.0
ParameterNumber|P_PSI|Wetting front suction [m]|None|None|0.2
ParameterNumber|P_DTHETA|Water content change across the wetting front|None|None|0.1
ParameterBoolean|BINF             |Green-Ampt Infiltration|True
OutputRaster|MOIST|Soil Moisture Deficit
OutputTable|TABLE|Simulation Output
