Catchment Area (Parallel)
ta_hydrology
ParameterRaster|ELEVATION|Elevation|False
ParameterRaster|SINKROUTE|Sink Routes|True
ParameterRaster|WEIGHT|Weight|True
ParameterRaster|MATERIAL|Material|True
ParameterRaster|TARGET|Target|True
ParameterNumber|STEP|Step|None|None|1
ParameterSelection|Method|Method|[0] Deterministic 8;[1] Rho 8;[2] Braunschweiger Reliefmodell;[3] Deterministic Infinity;[4] Multiple Flow Direction;[5] Multiple Triangular Flow Directon
ParameterBoolean|DOLINEAR             |Linear Flow|True
ParameterNumber|LINEARTHRS|Linear Flow Threshold|None|None|500.0
ParameterRaster|LINEARTHRS_GRID|Linear Flow Threshold Grid|True
ParameterRaster|CHDIR_GRID|Channel Direction|True
ParameterNumber|CONVERGENCE|Convergence|None|None|1.0
OutputRaster|CAREA|Catchment Area
OutputRaster|CHEIGHT|Catchment Height
OutputRaster|CSLOPE|Catchment Slope
OutputRaster|ACCU_TOT|Total accumulated Material
OutputRaster|ACCU_LEFT|Accumulated Material from _left_ side
OutputRaster|ACCU_RIGHT|Accumulated Material from _right_ side
OutputRaster|CASPECT|Catchment Aspect
OutputRaster|FLWPATH|Flow Path Length
