Analytical Hillshading
ta_lighting
ParameterRaster|ELEVATION|Elevation|False
ParameterSelection|METHOD|Shading Method|[0] Standard;[1] Standard (max. 90Degree);[2] Combined Shading;[3] Ray Tracing
ParameterNumber|AZIMUTH|Azimuth [Degree]|None|None|315.0
ParameterNumber|DECLINATION|Declination [Degree]|None|None|45.0
ParameterNumber|EXAGGERATION|Exaggeration|None|None|4.0
OutputRaster|SHADE|Analytical Hillshading
