Rasterization Application

Brief Description

Reproject and Rasterize a Vector Data.

Tags

Vector data Manipulation

Long Description

Reproject and Rasterize a Vector Data.

Parameters

- [param] InputVectorData (-in): The input vector data to be rasterized

- [param] OutputImage (-out): An output image containing the rasterized vector data

- [param] InputImage (-im): A reference image for extraction region and projection information (optional)

- [param] SizeX (-szx): OutputSize[0] (useless if support image is given)

- [param] SizeY (-szy): OutputSize[1] (useless if support image is given)

- [param] RSID (-epsg): Projection System RSID number (RSID 4326 for WGS84 32631 for UTM31N) (useless if support image is given)

- [param] OriginX (-orx): OutputOrigin[0] (useless if support image is given)

- [param] OriginY (-ory): OutputOrigin[1] (useless if support image is given)

- [param] SpacingX (-spx): OutputSpacing[0] (useless if support image is given)

- [param] SpacingY (-spy): OutputSpacing[1] (useless if support image is given)

- [param] Available RAM (-ram): Available RAM

Limitations

None

Authors

OTB-Team

See also

Example of use

- Parameters to set value:

- InputVectorData: Rasterization/polgons.shp

- OutputImage: rasterImage.tif

- SizeX: 1100

- SizeY: 1100

- Command line to execute:

otbcli_Rasterization -in Rasterization/polgons.shp -out rasterImage.tif -szx 1100 -szy 1100