Open Street Map layers importations applications

Brief Description

Generate a vector data from OSM on the input image extend

Tags

Image MetaData

Long Description

Generate a vector data from Open Street Map data. A DEM could be use. By default, the entire layer is downloaded, an image can be use as support for the OSM data. The application can provide also available classes in layers . This application required an Internet access. Informations about the OSM project : http://www.openstreetmap.fr/

Parameters

- [param] Output vector data (-out): Generated output vector data path

- [param] Support image (-support): Image used as support to estimate the models

- [param] OSM tag key (-key): OSM tag value to extract (motorway, footway...)

- [param] OSM tag value (-value):

- [param] DEM directory (-dem): Path to the directory that contains elevation information.

- [param] option to display available key/value classes (-printclasses): Print the key/value classes available for the bounding box of the input image ** If not used : Note that the options OSMKey (-key) and Output (-out) become mandatory

Limitations

None

Authors

OTB-Team

See also

Convertion

Example of use

- Parameters to set value:

- Output vector data: apTvUtOSMDownloader.shp

- Support image: ROI_QB_TOULOUSE.TIF

- OSM tag key: highway

- Command line to execute:

otbcli_OSMDownloader -out apTvUtOSMDownloader.shp -support ROI_QB_TOULOUSE.TIF -key highway