# Tutorial

This tutorial explains with an example how to create a new hydrogeologic model and how to create and use a new study.

Tutorial data can be found in the `thyrsis/tutorial_data` folder.

A hydrogeologic model is associated to a site and is a combination of a mesh and some scalar and spatial characterics.

The site can be characterized by points of interest, measurements and boreholes descriptions.

- Mesh creation
  - Mesh project
  - Meshing
- Model creation
  - Model parameters
  - Inversion
- Radionuclides
- Site characterization
  - Points of interest
  - Measurements
  - Boreholes
- Study creation
  - Computational database
  - Simulation parameters
  - Injection
  - Simulation and results