Highlights

- Spatially synchronized maps for each observation date
- Multiple band combinations in parallel, e.g. True Color and SWIR bands
- Multi-sensor support: separate render settings for separate senors/image products
- Visualization of Spectral and Temporal Profiles

Usage

1. "Files" > "Add images" to define the time series
2. "View" > "Add Map View" to create a new row of maps, e.g. for SWIR visualization
3. For each map view specifiy how each sensor should be rendered, e.g. RGB or single band color range
4. Optimize render settings, e.g. via map canvas context menu

Dependencies

- pyqtgraph (required)
- PyOpenGL (optional)

Install depencencies with `python -m pip pyqtgraph`