!_______________________________________________________
! GIS
Spatial Database == ..\model\gis\${model_name}_001.${gis_ext}
GIS Format == ${gis_format}
GRID Format == TIF
GPKG Projection == projection

!_______________________________________________________
! SOLVER
Tutorial Model == OFF
Solution scheme == HPC
Hardware == GPU

!_______________________________________________________
! SGS SETTINGS
SGS == ON
SGS Sample Target Distance == <distance>  ! TODO update to appropriate value based on model cell size

!_______________________________________________________
! SCENARIOS / EVENTS - Uncomment as required
! Model event == <event_name>
! Model scenario == <scenario_name>
! Event File == ..\model\${model_name}_events.tef

!_______________________________________________________
! CONTROL FILES - TODO uncomment as model is built (not all control files may be required)
Geometry Control File == ..\model\${model_name}_001.tgc
BC Control File == ..\model\${model_name}_001.tbc
BC Database == ..\bc_dbase\bc_dbase.csv
Read Materials File == ..\model\${model_name}_mat.csv
! Estry Control File == ..\model\${model_name}_001.ecf
! Read Soils File == ..\model\${model_name}_soils.tsoilf

!_______________________________________________________
! INITIAL WATER LEVEL - uncomment if required
! Set IWL == <Value>

!_______________________________________________________
! SIMULATION CONTROLS
Start Time == 0
End Time == <hrs>  ! TODO
! Timestep == <sec>  ! TODO uncomment if using Classic
! Timestep Initial == <sec>  ! TODO uncomment if using HPC
! Timestep Maximum == <sec>  ! uncomment if required (value should be based on cell size)

!_______________________________________________________
! OUTPUT FOLDERS
Log Folder == log
Output Folder == ..\results\
Write Check Files == ..\check\
! Write Check Files Exclude == ZPT GRD UVPT

!_______________________________________________________
! MAP OUTPUT FORMATS
Map Output Format == XMDF
Map Output Data Types == h v d q dt  ! TODO add data types as required
Map Output Interval == 3600  ! TODO update to appropriate interval for simulation duration

!_______________________________________________________
! MAP OUTPUT SETTINGS
SGS Map Extent Trim == All
SGS Depth Output == Cell Average
! Map Cutoff Depth == 0.01  ! uncomment if required

!_______________________________________________________
! PLOT OUTPUT - uncomment as required
! Time Series Output Interval == 60  ! TODO requires updating to sensible value to match simulation duration
! Read GIS PO == <path/to/2d_po>