location == TUFLOW Control File (.tcf)

command == Read GIS GLO

description == Used to define gauge level output (2d_glo) locations. The GLO command controls map output based on the height of the water at a specified location within the model domain.

wiki link == https://wiki.tuflow.com/TUFLOW_Empty_Files#TUFLOW_Control_file_.28TCF.29

manual link == https://docs.tuflow.com/classic-hpc/manual/2026.0/Outputs-1.html#GaugeLevel-3