location == BC Control File (.tbc)

command == Read GIS SA PO

description == The SA PO option models seepage or infiltration based on a varying water level or flow rate elsewhere in the model.

manual link == https://docs.tuflow.com/classic-hpc/manual/2026.0/Boundaries-InitialConditions-1.html#FlowFeature-4
