# This file should be included when you package your plugin.

# Mandatory items:


[general]
name=TUFLOW
qgisMinimumVersion=3.6
qgisMaximumVersion=4.99
supportsQt6=yes
description=A collection of utilities for TUFLOW flood and coastal simulation in QGIS
about=A collection of utilities for TUFLOW flood and coastal simulation in QGIS.
      Includes visualisation of results / inputs
      Editing tools
      Styling tools
version=2026.0.18
author=Phillip Ryan, Ellis Symons, Pavlina Monhartova
email=support@tuflow.com

# end of mandatory metadata

# Optional items:

# Uncomment the following line and add your changelog entries:
changelog=
          --- The changelog has been moved to the following URL ---

          <a href="https://docs.tuflow.com/qgis-tuflow-plugin/changelog/">docs.tuflow.com/qgis-tuflow-plugin/changelog</a>

          --- Older versions of the changelog are kept below for reference ---

          --- 3.10.2 ---
          - New Features and Enhancements -
          Run TUFLOW (Simple) - Adds option to capture console output in python
          Create Project (toolbox) - GPKG models use a Spatial Database format
          Create Project (toolbox) - Adds basic run batch file
          ARR to TUFLOW - Adds the option to add additional temporal patterns from both the point and areal temporal pattern sets
          TMO to Points - adds domain index (starting at 1) to point output

          - Bug Fixes -
          TUFLOW Viewer - Fixes NetCDF raster loading on Linux which was broken in v3.10
          TUFLOW Viewer - Bug fix to support SWMM 1D GPKG time-series files generated by simulations (tcf filename) which start with a number. Previously, these files would load but plotting would not work correctly
          Create Project (toolbox) - Adds missing bc_dbase.csv reference
          TUFLOW Plugin - Fixes an issue loading the plugin in older QGIS versions due to an illegal python statement for older python versions
          Convert TUFLOW Model GIS Format - Fixes bug that would not correctly give a CRS to the output GIS layers unless a user CRS was used
          Convert TUFLOW Model GIS Format - Fixes a bug when converting a model into a TUFLOW standard directory structure where .qcf was not recognised as a control file
          1D Integrity Tool - Fixes temporary layer creation from GPKG (removes fid attribute)

          --- 3.10.1 ---
          - New Features and Enhancements -
          TUFLOW Viewer - NetCDF rasters can be now be loaded without the Python netCDF4 library
          TUFLOW Viewer - 1D flow integral results now available if output from TUFLOW
          TUFLOW Viewer - 1D volume results now available if output from TUFLOW
          Convert TUFLOW Model GIS Format - Specifying an output folder will no longer add the root folder name to the output path
          Convert TUFLOW Model GIS Format - Add option to change the default TUFLOW directory structure (to some degree)

          - Bug Fixes -
          SWMM tools - Fixes bug that would stop plugin from loading due to dependencies
          TUFLOW Viewer - Fixes flow regime plotting for netCDF time series results
          TUFLOW Viewer - Fixes time series import for NC result format when the netCDF python library isn't present
          TUFLOW Viewer - Fixes bug when loading in NetCDF time series results without the water level output
          TUFLOW Viewer - When loading plot result gis layers, the path dividers will be corrected depending on operating system
          TUFLOW Viewer - Test bug fix when TUFLOW Viewer initialises temporal controller with an updated PyQt version (PyQt is stricter with data types)
          Load Layers from TCF - Quadtree single level is no longer reported as an error
          Convert TUFLOW Model GIS Format - Output projection file will now be written correctly when forcing projection
          Load From TCF - Fixes bug loading inp files from TSCF
          Load From TCF - Fixes bug where an uninitialised variable could be hit

          --- 3.10 ---
          - New Features and Enhancements -
          TUFLOW Viewer - Adds GPKG time series results (currently written by TUFLOW-SWMM)
          TUFLOW Viewer - Disable matplotlib 3.5.1 "legend about to break" check and message
          TUFLOW Viewer - Selecting 1d node results will no longer affect any 1d long section results
          TUFLOW Viewer - unchecking a mesh layer in the Layers Panel will no longer unselect the corresponding result in TUFLOW Viewer
          TUFLOW Viewer - SWMM gpkg time series format is not supported within load from TCF/TLF functions
          TUFLOW Viewer - NetCDF rasters and GPKG time series working in animation export tool
          TUFLOW Viewer - Implemented new reload data functionality using copied results which stops conflict between TUFLOW and QGIS if simulation is still running
          TUFLOW Viewer - User option to delete copied results on close. Button to delete all copied results added.
          Load From TCF - Commands where no files are loaded are now reported
          Configure TUFLOW Project (toolbox) - Updates HPC template control files with missing commands
          Toolbox - Adds new tool 'Create CN Lines' - port of mitools 'Create TUFLOW CN Lines' tool
          Toolbox - Adds new tool 'Create Cross-Section Lines' - port of mitools 'Create TUFLOW XS' tool
          Toolbox - Adds new tool 'Create Water Level Lines' - port of mitools 'Create TUFLOW WLL' tool
          Toolbox - TUFLOW-SWMM Tools added
          Import Empty Toolbox - Empty directory can point to either the Project folder or Empty Directory
          Import Empty - Adds 2d_wrf tooltip
          GPKG time series styling added to GIS layer context menu
          Copy TUFLOW Command - A little more clever when searching for control files in case it finds an erroneous 'TUFLOW' folder

          - Bug Fixes -
          TUFLOW Viewer - Fixes bug where Flood Modeller cross-sections weren't plotting due to the change in inactive area handling in TUFLOW Plugin v3.9
          TUFLOW Viewer - Fixes bug when loading a cross-section that starts with a valid float number in the header
          TUFLOW Viewer - Fixes python error that prevented TUFLOW Viewer from loading when there was a 1d_xs
          TUFLOW Viewer - Fixes hover over plot labelling for matplotlib 3.7
          TUFLOW Viewer - fixes a bug that stopped loading tpc result when a '#' was present in the flow regime result
          TUFLOW Viewer - Removes duplicate result types from 2d_bc_tables
          TUFLOW Viewer - Static NetCDF grid results no longer affect the time slider
          TUFLOW Viewer - Optimised code relating to feature selection when viewing time series results
          TUFLOW Viewer - Long profile results are not shown if only 2D results are available (Time Series results)
          Load from TCF - Fixes python error that would occur if an xf layer was being referenced
          Arch Bridge Editor - Fixes bug where the tool would error when running if features were drawn and saved while the editor was open
          1D Integrity Tool - Fixes bug where a cover limit of exactly zero wasn't flagging any cover issues
          1D Integrity Tool - More robust recognition of 1d nwk layers
          1D Integrity Tool - Fixes Python error that could occur when loading layers into a workspace with raster layers
          1D Integrity Tool - Vector layer input comboxes will no longer reset if a layer is added/removed from workspace
          1D Integrity Tool - Error is shown to user if selected channels are not connected when using the flow trace tool. Previously this would error silently and progress bar looked to hang.
          1D Integrity Tool - Remembers selected DEM which could reset if layers were added/removed from workspace
          1D Integrity Tool - Fixes python error that could occur if an aerial image was accidentally used as ground surface
          Import Empty (Toobox) - Fixes bug that could potentially not correctly bring in new GPKG layer if GPKG contained more than one layer
          Import Empty (Toolbox) - Removes duplicate empty types from list
          Apply GPKG Name - Fixes bug where name wasn't applied to raster layers where the database only containes one raster layer
          Increment Layer - Fixes bug that would cause python error if a layer group was selected
          Convert TUFLOW Model GIS Format - Fixes bug on tool initialisation when using network drivers (caused python error)
          Run TUFLOW - Fixes bug that can cause Python error when browsing for TUFLOW.exe

          --- 3.9 ---
          - New Features and Enhancements -
          TUFLOW Viewer - Adds BC tables check file (1D)
          TUFLOW Viewer - Animation supports user defined time formatting
          TUFLOW Viewer - Flood modeller results can now be shown on cross-section even if they don't intersect the PLOT_P points if they have the same name
          ReFH2 to TUFLOW - Rainfall model FEH2022 now supported in tool
          TUFLOW Plugin Downloader - Adds button to copy the download path to the clipboard
          Increment Layer - New tool in layer context menu (new tools but similar to existing import empty tool)
          Import Empty - New tool in TUFLOW processing toolbox (very similar to existing import empty)
          Create Project - New tool in TUFLOW processing toolbox (very similar to configure project)
          Adds new/missing empty types to the empty tooltips (2d_bg, 1d_bg, 1d_lc)
          Adds Filter Message by ID to TUFLOW context menu for messages_P layers
          Adds TUFLOW Context menu to QGIS Layers Panel
          Adds 'Copy TUFLOW Command' tool to TUFLOW context menu
          Package Model - Package Model (using TUFLOW.exe) added to the TUFLOW toolbox
          TUFLOW Utilities - GPKG rasters now supported when adding opened layers
          Apply GPKG Layer Names - GPKG rasters now supported
          Load from TCF - Older style 'ESTRY CONTROL FILE AUTO' syntax now supported
          SWAN GIS - updated version to latest available
          Style Current Layer - _ccA_L result file now has default styling
          ARR to TUFLOW - LIMB data will now be processed if available
          ARR to TUFLOW - Removes longitude limit (>153.2999)
          Incremenet Layer - Adds user check when overwriting an existing layer in a GPKG

          - Bug Fixes -
          TUFLOW Viewer - Time series results are now loaded correctly using 'utf-8' encoding which enables handling of special characters
          TUFLOW Viewer - Loading NetCDF Grids will now try and load all selected layers before reporting errors
          TUFLOW Viewer - Results with only maximums will now appear in relevant plot menus
          TUFLOW Viewer - fixes loading netCDF raster as mesh
          TUFLOW Viewer - XS deactivation was only working when using the MAT approach
          TUFLOW Viewer - Loading mesh layers on when TUFLOW Viewer is opened was getting tangled if layers of different types (vector layers / mesh layers) had the same name
          TUFLOW Viewer - Fixes flood modeller result cross-sections not loading when X,Y coordinate did not contain a space between them in DAT file
          TUFLOW Viewer - Fixes animations with embedded plots not working in QGIS 3.30
          TUFLOW Viewer - Fixes bug introduced in 3.8.2 that prevented NetCDF grid results from being loaded (produced python error about missing 'events' argument)
          TUFLOW Utilities - Fixes bug in asc_to_asc brkline tool where the vector layer was being passed into the utility instead of the raster layer
          TUFLOW Utilities - Fixes bug where no 'browse' buttons were working
          TUFLOW Utilities - Downloader was hanging indefinitely due to a python error on a separate thread in QGIS 3.32 (caused by new numpy version)
          Configure Project - Fixes bug that would not correctly save empty file location for TUFLOW FV
          TUFLOW Styling - Fixes default styling for sac_check_R
          TUFLOW Styling - ISIS 1d_nwk layers are now given a single styling previously would cause python error because they are not guaranteed to have the standard 1d_nwk fields
          Convert Model GIS Format - Fixes bug that cause new filepaths to be incorrect when convert filename that were only a number (e.g. 001.tgc)
          Load from TCF - fixes bug that would not load layers if brackets were included in file path
          Load from TCF - fixes issue that would cause a python error if there was a '|' at the end of a GIS input command


          --- 3.8.2 ---
          - New Features and Updates -
          Load from TCF - Adds new option to load layers sorted by control file order (exactly or group raster separately)
          Load From TCF - Layers inside an 'IF Event' logic block will now be available for selection - previously only 'IF Scenario' options would be available to the user
          Load from TCF - Keep blue highlighting in selection widgets even when they lose focus
          Import Empty - Adds 'Import into Kart Repo' option

          - Bug Fixes -
          TUFLOW Viewer - Fixes bug that could cause strange plotting behaviour when 1D/2D results were both loaded and the reference time was changed for the 2D results
          TUFLOW Viewer - not always picking up 1d_xs layers from GPKG
          TUFLOW Viewer - Fixes bug that would sometimes not show all available groundwater PO outputs
          TUFLOW Viewer - Fixes bug that could cause python error when trying to close a result just after TUFLOW is started overrided the same result layer
          Load from TCF - Fixes bug that could cause a load error if the output folder was a Windows path variable
          Load From TCF - MIF layers with 2 geometry types will now correctly load in line types which could sometimes not load in correctly
          ReFH2 to TUFLOW - Fixes tool not initialising correctly when plugin is loaded which was causing 'unexpected' error when the tool was opened by user
          Arch Bridge Editor - fixes bug that would not recognise GPKG input layers as 1d_nwk
          1D Integrity Tool - fixes python error that could occur if no points where included when running the snapping tool
          1D Integrity Tool - Fixes bug that could cause python error due to non-unique indexing internally
          Increment Layer - Fixes a bug that would lead to strange autofilled increment names (or python errors) when the source layer name was using letters along side version number e.g. '002b'
          Configure Project - Updates to latest vector file creation functions in QGIS. Projection.shp causes error in QGIS 3.30

          --- 3.8.1 ---
          - Bug Fixes -
           TUFLOW Viewer - A rogue import statement was causing the plugin to not load
           TUFLOW Viewer - fixes bug that would not correctly update newly selected result in open result widget
           TUFLOW Viewer - fixes bug when importing results from TCF when some input layers are using absolute path references that could cause a python error
           TUFLOW Viewer - No longer prompt user about saving default styles - could prompt (many times) when saving a project
           TUFLOW Toolbox - tmo_to_points wasn't being loaded
           Utilities - Fixes issue when running 'info' function and non-ascii characters are logged which may cause the tool to error

          --- 3.8 ---
          - New Features and Updates -
          Adds latest available development version to 'About' dialog
          Adds downloader for latest available development version
          TUFLOW Viewer - Updates saving/loading vector styles to include streamlines and flow traces. Not backward compatible and will not load old styles
          TUFLOW Viewer - Load results from TCF - Handles encoding errors
          TUFLOW Viewer - Workaround added for TUFLOW FV NetCDF mesh outputs that now properly renders velocity maximums
          TUFLOW Viewer - Adds axis labels for 1D hydraulic tables
          TUFLOW Viewer - Adds ability to flip which axis is using a secondary axis
          TUFLOW Viewer - Adds (xs) or (nwk) to hydraulic table results to indicate which input layer should be selected to view hydraulic property
          TUFLOW Viewer - Animation export format default changed to MP4
          TUFLOW Viewer - Better error handling added to FFMPEG downloader. Previously if download process crashed it sometimes didn't report anything and it looked like it was hanging
          TUFLOW Viewer - Now possible to copy a result type style into multiple results
          TUFLOW Viewer - Adds result name to filename for the cross-section batch plot export. Similar to the time series batch export filenames.
          TUFLOW Viewer - NetCDF grid results now have option to change reference time
          TUFLOW Viewer - visibility of results now try and communicate with QGIS layers panel and tries keeps them in sync (i.e. checked / unchecked) - fixes potential issue in QGIS 3.28 where they can go out of sync after using the F7 panel
          Load From TCF - Catch errors when loading layer from TCF
          Load From TCF - Handles encoding errors
          Style Current Layer - Adds bg_uvpt_check
          TUFLOW Utilities - Adds breakline function to 'common' utilities
          TUFLOW Utilities - Adds ASC_to_ASC version to utility
          TUFLOW Utilities - Adds output format option to ASC_to_ASC utility for 2023 version
          Increment Layer Tool - Added new GPKG option to save a superseded version of layer so working copy can be modified
          Configure Project - Dialog will will only close if the tool runs successfully

          - Bug Fixes -
          Removes most of the "sys.path.append" calls in the code. This should make it less likely to get tangled with other plugins or python libraries
          Fixes bug that was not correctly unloading a couple of the tools
          TUFLOW Viewer - Fixes 1D xs viewing when using a GPKG layer
          TUFLOW Viewer - No longer recognised 1d_bc as a 1d_tab type
          TUFLOW Viewer - Fixes Minimum dt display in QGIS 3.30 - now should correctly display as only one result type
          TUFLOW Viewer - Fixes bug that would not load 1D results correctly on project load
          TUFLOW Viewer - Fixes bug that could retain feature selection in layers that were removed or otherwise deselected
          TUFLOW Viewer - Fixes a bug with plotting 1D cross-sections that would cause them to be plotted even though the 'XZ' type was not selected
          TUFLOW Viewer - Fixes a bug with plotting 1D cross-sections that would stop them from being plotted after switching to a different plotting tab then coming back to the cross-section plotting tab
          TUFLOW Viewer - Fixes a bug that would not plot cross-section hydraulic tables if the 1d_xs and source CSV were in different folders
          TUFLOW Viewer - Fixes a bug that could cause switching between results to be really slow if multiple 1D results were loaded at the same time
          TUFLOW Viewer - NetCDF grids are now correctly saved / loaded in qgis project
          TUFLOW Viewer - fixes 'Move down' option when there are only 2 results open
          TUFLOW Viewer - Fixes python error that could occur if selecting channel results when another open result only contains 2D PO results
          TUFLOW Viewer - Fixes grammatical error in batch export map tool successful message box
          TUFLOW Viewer - Fixes python error that could occur when batch exporting plots when data was of different lengths
          1D Integrity Tool - Fixes X connectors not being properly handled when using flow trace tool
          1D Integrity Tool - Fixes spelling mistake in Continuity Tool description
          Import Empty - Fixes bug that would cause 'convert to database' always to be checked when QGIS is first opened - now correctly remembers previous setting between sessions
          Increment Layer Tool - Fixes bug that would update a layer's name in layer panel but not the data source if an incremented layer had duplicates in the project
          Increment Layer Tool - Fixes bug that would display "|layername=" for shp files after using 'import from tcf' tool
          Convert TUFLOW Model GIS Format - Fixes bug that would not correctly convert TCF commands prefixed with '1D'
          Convert TUFLOW Model GIS Format - Fixes a bug that would cause the tool to not bring in all layers if a scenario name had a decimal point in the name (e.g. If Scenario == 2.5m)
          Configure Project - Fixes bug that would not cancel tool after user cancel request

          --- 3.7 ---
          - New Features and Updates -
          Arch Bridge Editor - new tool
          TUFLOW Viewer - Changing rendering style of a result type will now also change the style of the maximum and minimum type of the same name (and visa versa)
          TUFLOW Viewer - Support reloading of mesh layers (must use reload layer tool if results have changed otherwise QGIS crashes)
          TUFLOW Viewer - Increased hover over label speed. From testing 10,000 point dataset: prev. each label took ~1.0s to calculate and render, now = ~0.15s
          TUFLOW Viewer - Adds units and label to y-axis for RFR, RFC, RFML outputs
          TUFLOW Viewer - Adds 'Water Level' and 'Max Water Level' result types to cross-section (previous had to use time series 'Level' result type)
          ARR to TUFLOW - Will download point temporal pattern CSV manually if no temporal patterns are found in the ARR_Web_Data.txt
          ARR to TUFLOW - CSV output now includes event id
          Import Empty - Database settings are now saved from previous tool runs
          Reload Layer - Updated to support mesh layers in QGIS 3.28+
          Load From TCF - Improved progress bar
          Load From TCF - Adds ability to select any TUFLOW control file to import from
          Convert Model GIS Format - Adds ability to specify output CRS
          Convert Model GIS Format - Tool will now log commands that do not convert/copy any files (but should do)
          Convert Model GIS Format - Adds option to create empty files for converted model
          Convert Model GIS Format - Adds option to specify the output GPKG database name when using a grouped profile
          Processing Toolbox - Added 'TMO to Points' algorithm
          Adds file encoding prediction for all tools that read from the TCF and other control files

          - Bug Fixes -
          TUFLOW Viewer - Fixes a bug that would cause python error and not display results when trying to plot TS_P.shp and TPC results at the same time
          TUFLOW Viewer - Fixes bug when saving project when a TS_P.shp was loaded that could cause a python error
          TUFLOW Viewer - fixes rendering map outputs in QGIS 3.28 which could become scrambled if min dt was present (a bug is still present in QGIS that no longer renders temporal min dt)
          TUFLOW Viewer - Fixes bug that would incorrectly carry over 1D result types to next loaded result dataset
          TUFLOW Viewer - Stops duplicate plots of the same 1D element - can happen if the PLOT layer is duplicated in the workspace
          TUFLOW Viewer - Fixes bug that would produce python error after closing mesh results from layers panel then trying to close 1D results
          TUFLOW Viewer - Fixes bug in Load from TCF when a scenario name contains dashes (-)
          TUFLOW Viewer - fixes bug in map output flow calculation which was producing a python error
          TUFLOW Viewer - Fixes python error that could occur after closing tuflow completely and re-opening with time series result when a PLOT feature is already selected
          TUFLOW Viewer - Unidirectional pipes now plotted correctly in long plot
          TUFLOW Viewer - cell centre 'bed elevation' results in TUFLOW FV netCDF format will no longer check if face is active in plot window
          TUFLOW Viewer - Load from TCF now correctly finds output zone results
          TUFLOW Viewer - Fixes bug that would cause 1D long sections to not plot when 1D point objects were also selected
          TUFLOW Viewer - Fixes bug when viewing results on cross-sections with mif files that would not show water levels
          TUFLOW Viewer - Fixed bug in animation tool that could cause python error if the dataset was the first in the mesh layer (index = 0)
          1D Integrity Tool - fixes python error that could occur when checking for non-compliant channel ids in QGIS 3.26
          1D Integrity Tool - Fixes bug in Unique Channel ID tool that wasn't correctly flagging non-compliant ids
          Configure Project - Fixes bug that would not create empties if 'Create Model Folder Structure' was not also ticked
          Increment Layer Tool - Handles empty geometry layers a little nicer
          Import Empty - Fixes 'Convert to GPKG' option which wasn't doing anything
          Insert TUFLOW Attributes - Fixes insert '2d_mat' when using GPKG
          Style Current Layer - Fixes tooltip
          Load From TCF - Fixes a bug that did not load layers from ECF if using "Estry Control File == AUTO"
          TUFLOW Utilities - info tool will error gracefully if an error occurs with the utility
          TUFLOW Utilities - Fixes browse dialogs hanging if previous file/folder path was on a drive that is no longer connected
          TUFLOW Utilities - Fixed bug that would crash QGIS if the download button is clicked twice in a row
          TUFLOW Utilities - Cache is now cleared for download links so latest is always downloaded

          --- 3.6 ---
          - New Features and Updates -
          TUFLOW Viewer - Curtain vectors will now have a vertical component if 'W' output is found in results
          TUFLOW Viewer - Added option to shift order of open results via right-click context menu
          TUFLOW Viewer - Added 'Remember Previous State' layout option
          TUFLOW Viewer - NetCDF grids now supported
          TUFLOW Viewer - Adds Python exported CSV format for flood modeller time series results
          TUFLOW Viewer - Adds ZZN support for flood modeller time series results
          SCS to TUFLOW - SCS method calculated from GIS polygons
          Load From TCF - Added progress bar
          Load From TCF - Imported layers are automatically given TUFLOW styling
          Load From TCF - Option to bring in layers 'grouped' or 'ungrouped'
          Sort/Filter Layers - Improved speed and altered sorting algorithm slightly so that layers with the same name (w/o '_L', '_P', '_R' suffix) will be sorted by geometry in order of points, line, polygon
          Convert Model GIS Format - Provides user with the option to restrict conversion by scenario name
          Configure Project - New icon and added to toolbar
          TUFLOW Styling - Added styling for 2d_qnl
          TUFLOW Utilities - TUFLOW to GIS will automatically find 2dm if using a post-processed XMDF

          - Bug Fixes -
          TUFLOW Viewer - Cross-section plot lines could become offset if start or end of line was outside the mesh
          TUFLOW Viewer - Fixes bug for long section plotting of Flood Modeller results that could sometimes produce a python error
          TUFLOW Viewer - Fixes bug in hiding inactive area on cross-section when M column header isn't defined in GIS file
          TUFLOW Viewer - Fixes bug with cross-section plot that wouldn't update plot when a result type was deselected
          TUFLOW Viewer - Fixes bug when loading results from TCF which could produce a python error when ~s~ flag was just before extension .tcf in the name
          TUFLOW Viewer - Fixes 'load results from TCF' when output path is an absolute path
          TUFLOW Viewer - Fix bug when loading TUFLOW release 2013 time series results which could produce a python error
          TUFLOW Viewer - New method for loading results from TCF backported to be compatible with Python versions earlier than 3.9 and QGIS versions earlier than 3.22
          1D Integrity Tool - Fixes a bug with the ouput symbol renderer in QGIS 3.26
          TUFLOW Utilities - Fixes bug with TUFLOW to GIS common tool using correct scalar/vector type and loading timesteps from a post-processed XMDF
          TUFLOW Styling - Fixes a bug that would not render TUFLOW style for GPKG layers
          Import Empty - Fixes a bug where open layers with the same name as the imported layer were removed from the workspace
          ReFH2 to TUFLOW - Fixes bug that would cause GUI to hang if 2 different output types (within rainfall or hydrograph) was selected (e.g. Direct Runoff and Total Runoff)
          ReFH2 to TUFLOW - Fixes python error that could occur if the selected GIS layer was removed
          Load From TCF - Fixes bug in new routine that wasn't finding all scenario names

          --- 3.5.1 ---
          Convert Model GIS Format - Updates to the latest version

          - Bug Fixes -
          ARR to TUFLOW - removes remote debugging breakpoint added in 3.5 which was causing crash.

          --- 3.5 ---
          - New Features and Updates -
          Load From TCF - new feature - user has option to load rasters, not load rasters, or load them but don't render them
          TUFLOW Viewer - Load results from TCF now finds results that have appended scenario names
          TUFLOW Viewer - changed extension order in browser dialog for load map outputs (xmdf is now listed first)
          ARR to TUFLOW - Sets initial losses > 72hrs to the 72 hr initial loss value

          - Bug Fixes -
          Auto Label - Fixes auto label tool in QGIS 3.26
          TUFLOW Viewer - fixes animation export
          Import Empty - ensures the .prj file of the imported empty is the same as the empty - this was previously implemented but was recently broken in v3.4
          Configure Project - Was not correctly setting the empty directory in the Import Empty and Insert TUFLOW Attributes tool if the 'Save to Project' or 'Save Globally' was used in either tool.
          ARR to TUFLOW - Fixes a bug when selecting 'Use Event Independent Continuing Losses' that would cause the variable setting TRD file to become scrambled.

          --- 3.4 ---
          - New Features and Updates -
          Added New Stability Styling tool - new button is located using dropdown arrow under 'Style Current Layer' button
          TUFLOW Viewer - added ability to 'quick view' _TS output GIS layers. Not full featured (no axis names, does not populate time slider, no secondary axis etc)
          TUFLOW Viewer - User option added to view/hide inactive areas in 1D cross-sections
          TUFLOW Viewer - Cross-section source reference with a leading '/' will now be interpreted the same as './'
          TUFLOW Viewer - animation exporter will now update temporal properties of all map windows (allows for insets)
          1D Integrity Tool - Now produces a warning instead of an error if the input layer doesn't look like a 1d_nwk type
          ARR to TUFLOW - If storm loss values are NaN from the datahub, the tool will now assume zero and produce an error message for the output log file
          ARR to TUFLOW - Added additional columns ("Storage Reduction Factor" and "Fraction Impervious") to material.csv output
          TUFLOW Styling - added custom styling for VZSH_ZPT_CHECK
          TUFLOW Styling - NWK_C check styling now has purple "all else" style visible by default
          TUFLOW Utilities - Increased width of timesteps combobox for "TUFLOW to GIS" common tools

          - Bug Fixes -
          TUFLOW Viewer - fixed bug that caused map to not update when clicking different result types after loading from a project
          TUFLOW Viewer - was converting all length units to metres for 2D/3D cross-section plotting. Will now use map canvas units
          TUFLOW Viewer - fixed a bug that would incorrectly show the maximum water level on 1D cross-sections
          TUFLOW Viewer - New method of loading result from TCF was sometimes incorrectly loading in results that weren't selected by the user
          Import Empty - Fixed bug when choosing option to 'Convert to GPKG' that wouldn't correctly create a GPKG layer with TUFLOW attributes or projection
          Load Layers From TCF - fixed loading GPKG layers that would sometimes fail to load
          Configure Project - Fixed 'OK' button that was disabled within the select CRS dialog

          --- 3.3---
          - New Features and Updates -
          GPKG compatibility added to relevant tools - Functionality added for the 2022 TUFLOW release - keep watch for beta release coming soon!
          Processing Toolbox - Added TUFLOW Processing Toolbox
          Processing Toolbox - Added "Convert TUFLOW Model GIS Format" script
          TUFLOW Viewer - New approach when loading from TCF - all possible results listed to user rather than possible scenarios. Old method still available via Settings > Defaults.
          TUFLOW Viewer - cross section / long plots in animation now gives user options to set axis limits different ways. Opening plot properties will no longer trigger axis limit calculation which could sometimes take a while.
          TUFLOW Viewer - added hover over channel names to 1D results for long plotting - similar to culvert hover over labelling
          TUFLOW Viewer - use blitting to make hover over labelling a lot quicker and hopefully now feels 'snappier'
          TUFLOW utilities - TUFLOW to GIS now has option to load header information from an XMDF file to populate available result types and timesteps
          Apply GPKG Names - New Tool - renames GPKG layers in QGIS Layers Panel to match their name in the GPKG database
          Auto Styling - now supports GPKG layers
          Import Check Files - now supports check files written as GPKG
          Import Empty - now supports GPKG empty files and an option to convert SHP empty file to GPKG
          Insert TUFLOW Attributes - now supports GPKG empty files and an option to convert SHP empty file to GPKG
          Configure Project - now supports GPKG option (requires TUFLOW 2022 release)
          About Dialog - now has QGIS and Python version also listed for convenience
          1D Integrity Tool - Added additional 'magnitude' column to 'output' GIS layer that defines how far big the error is based on respective tool (bigger magnitude = bigger issue)
          1D Integrity Tool - Added auto symbology for the 'output' GIS layer that uses a graduated size based on the 'magnitude'
          1D Integrity Tool - styling is automatically applied to 'output' layer
          1D Integrity Tool - option will be given to automatically replace inputs with tool outputs after running certain tools
          1D Integrity Tool - updated GUI with links to documentation and reduced the height
          1D Integrity Tool - output tmp layers automatically copy the style of input layers
          1D Integrity Tool - Significantly improved the speed of the long plot generator in the flow trace tool - will be most noticeable on big datasets
          1D Integrity Tool - Can now limit flow trace and long plot to particular section of network by selecting 2+ channels to connect between
          1D Integrity Tool - long plot - added basic plotting tools and interaction
          1D Integrity Tool - long plot - hover over labelling now shows more information on the channel
          1D Integrity Tool - long plot - hover over labelling now shows more information on continuity flags
          1D Integrity Tool - long plot - added export/copy data options in context menu
          1D Integrity Tool - long plot - can toggle legend on/off in context menu
          1D Integrity Tool - long plot - can toggle continuity flags on/off in context menu
          1D Integrity Tool - long plot - current pipe at mouse position is shown in QGIS map window
          1D Integrity Tool - long plot - can zoom to current channel in map window using context menu
          1D Integrity Tool - long plot - can zoom to selected path extent using context menu
          1D Integrity Tool - long plot - pipe labels now try and avoid overlapping

          - Bug Fixes -
          TUFLOW Viewer - prevent scrambling of datasets in plot window due to bug in matplotlib 3.5.1 (packaged with QGIS 3.24.1)
          TUFLOW Viewer - colour bar is now always displayed for curtain plot (if legend is on) - previously if there was no data (i.e. section was dry) the colour bar wasn't shown. Mostly affects animations.
          TUFLOW Viewer - fixed colour bar label which broke with an update to the matplotlib library
          TUFLOW Viewer - TUFLOW FV XMDF outputs now will correctly show maximums
          TUFLOW Viewer - Fixed bug that could cause Python error if _PLOT_ layers were removed from workspace while TUFLOW Viewer was closed
          TUFLOW Viewer - Fixed bug with icon size setting introduced in v3.2 for QGIS versions < 3.16 that would cause error when trying to load
          TUFLOW Viewer - Hover over labelling is broken in latest QGIS python/matplotlib version - now fixed
          TUFLOW Viewer - fixed bug that could occur when loading from a qgz/qgs
          ReFH2 Tool - fixed bug that broke ReFH2 GUI from opening in previous release
          Import Empty - TUFLOW empty type list will be properly updated after user uses 'browse' to select a directory
          Insert TUFLOW attributes - TUFLOW empty type list will be properly updated after user uses 'browse' to select a directory
          Configure Project - Displayed paths now show correct operating system slashes
          TUFLOW utilities - Common functions - can now specify an output name without specifying an output directory
          TUFLOW utilities - Common functions - output name in TUFLOW_to_GIS was not working
          1D Integrity Tool - No longer need a line layer to check for empty geometries in points or cross section layers
          Load From TCF - Will now load layers from 'Create TIN Zpts' command
          Auto Label - Fixed tooltip when mouse hovers over toolicon in plugin toolbar
          SCS Tool - now unloads properly
          TUFLOW Menu under Plugins - now unloads properly


          --- 3.2 ---
          - New Features and Updates -
          TUFLOW Viewer - Added option to copy and paste scalar and vector styling within TUFLOW Viewer
          TUFLOW Viewer - Icon size can now be changed in TUFLOW Viewer > Setting > Options
          TUFLOW Viewer - Icon size should be corrected for Ultra HD monitors
          TUFLOW Viewer - Hover over pipe labels added to cross-section plotting tab
          TUFLOW Viewer - Long sections from 1D results now allow users to generate sections along non-primary flow paths by selecting an upstream and downstream section to go between
          TUFLOW Viewer - If cross-section CSV is missing, copying the CSV to correct location and refreshing the plot will now correctly reload from CSV
          TUFLOW Viewer - Added icons to plotting tab headings. Changed long-profile icon for time series results to be the cross-section icon
          1D Integrity Tool - Added new tool: Empty Geometry (find and fix)
          1D Integrity Tool - Added new tool to find and fix duplicate IDs or empty IDs
          1D Integrity Tool - Added check in most tools that stops the tool from running if there are duplicate or empty IDs as this can cause errors or funny behaviour in most of the tools
          1D Integrity Tool - Gave all output layers a consistent naming convention - 'original_lyr_name_tmp'
          Import Empty - Tooltips updated to include some missing empty types and updated to link to the 2018 Manual.
          Import Empty - User can now save the current empty directory to the project or globally
          Auto Labelling - Added _PLOT_L and _PLOT_P custom label rules
          Insert TUFLOW Attributes - User can now save the current empty directory to the project or globally
          Load From TCF - Now supports GPKG vector and raster format
          Load From TCF - Now supports TIF raster format
          TUFLOW Styling - Added 2d_rf style
          TUFLOW Styling - Updated 2d_sa style with to have more transparency

          - Bug Fixes -
          TUFLOW Viewer - Save default style fixed
          TUFLOW Viewer - Load scalar and vector datasets correctly for xmdf results outside of velocity and unit flow
          TUFLOW Viewer - Fixed bug in time series results that could load groundwater results incorrectly as surface results e.g. 'groundwater level' as 'level'
          TUFLOW Viewer - Fixed bug that could cause python error or unusual plotting behaviour if time series results was removed then re-added with updated/different output types
          TUFLOW Viewer - Fixed bug that user to have to deselect result in 'Results' list a couple of times to toggle it off after loading time series results only [similar to bug fixed in 3.1.10]
          TUFLOW Viewer - Fixed bug that would cause Python error when plotting 'US Level' or 'DS Level' when a point object from PLOT_P was also selected
          TUFLOW Viewer - Default font size is now correctly shown in options dialog after it is changed without having to restart TUFLOW Viewer
          TUFLOW Viewer - Fixed bug that could occur when loading from a project can cause Python error when time series results are in the project
          TUFLOW Viewer - Fixed bug that could cause water level results to not appear on cross-section
          TUFLOW Viewer - Fixed bug for viewing cross-section that would not correctly handle column names in the GIS layer
          TUFLOW Viewer - Time series long plot will now check for circular references in the 1D channel system. Previously this could cause QGIS to hang.
          Import Empty Tool - Fixed and issue where older versions of QGIS (older than 3.10.3) had stopped working due to the use of new modern methods.
          Increment Layer Tool - Fixed and issue where older versions of QGIS (older than 3.10.3) had stopped working due to the use of new modern methods.
          TUFLOW Styling - Fixed bug that would cause a Python error if no layer was selected
          Load from TCF - Fixed bug that would cause Python error when a command had '==' as a comment.

          --- 3.1.10 ---
          TUFLOW Viewer - Cursor location on cross-section plot is now projected onto map canvas
          TUFLOW Viewer - Added hover over labels on curtain plot
          TUFLOW Viewer - Fixed load from TCF that would fail if more than 2 variables were used in a row in output folder name
          TUFLOW Viewer - Fixed bug that could cause QGIS to crash when removing particle and map output results from Layers Panel at the same time
          TUFLOW Viewer - Active result type(s) are now retained as 'off' if the result is toggled in the 'Results' list
          TUFLOW Viewer - Active time is retained if the result is toggled in the 'Results' list
          TUFLOW Viewer - Fixed bug that could cause result type not to render if maximum value was toggled on in a previous open result and current result does not contain a maximum
          TUFLOW Viewer - Fixed bug that user to have to deselect result in 'Results' list a couple of times to toggle it off after loading from a project file
          TUFLOW Viewer - Particle results are now only displayed if the result is selected in 'Results' list
          TUFLOW Viewer - Fix bug that could cause QGIS to crash on close if particle results were loaded with map output results
          TUFLOW Viewer - Fix bug that would cause curtain plot colour bar legend to not show if there was a result on the secondary axis
          TUFLOW Viewer - Curtain plot colour bar will now be removed if the user toggles off legend
          TUFLOW Viewer - Fix bug that could cause hydraulic table to display properties from incorrect channel
          TUFLOW Viewer - Sped up curtain plots on xmdf / dat results by saving bed elevation data after first plot
          TUFLOW Viewer - Fixed bug that could occur sometimes when selecting/deselecting result types that would cause some muddling of plotting and displayed results
          TUFLOW Viewer - Fixed bug in hover over label routine that would sometimes cause plot to relimit when user's mouse enters the plot area
          TUFLOW Viewer - Fixed bug where unrecognised flow regime typese would cause python error - more types inlcuded, but won't error when encounters unknown
          TUFLOW Viewer - Added units on axis name for sediment, Q SED, Q TRACE, Q SALT
          TUFLOW Viewer - Updated hover snapping to hopefully be nicer - will check other datasets for closer values (previously would stop at first found)
          TUFLOW Viewer - Different Time Series geometry types can be viewed at the same time now - e.g. flow from 2d_po line and level from 2d_po point
          TUFLOW Viewer - Fixed bug loading time series where timesteps were sometimes being loaded incorrectly
          TUFLOW Viewer - Sped up curtain plot updating (e.g. updating the time) a little by saving mesh interesects / faces
          TUFLOW Viewer - Added TUFLOW FV time series outputs
          Load from TCF - Quadtree control file will now be loaded
          TUFLOW Styling - Fixed _sac_check_R style

          --- 3.1.9 ---
          TUFLOW Viewer - Added hover-over labelling on plots
          TUFLOW Viewer - Toggling 'Show as Dates' will no longer reload default mesh styles - previously this would override any changes in style the use had made to the mesh
          TUFLOW Viewer - Toggling 'Show as Dates' could sometimes badly relimited curtain plot axis if the Long Plot plot wasn't the active plot when toggled
          TUFLOW Viewer - Curtain plot retains colour bar name changes
          TUFLOW Viewer - Cross section / long profile plot will now correctly reset user colour changes (when requested through the View menu)
          TUFLOW Viewer - Fixed bug in FM time series import
          TUFLOW Viewer - 3D to 2D depth average time series plotting working again
          TUFLOW Viewer - Curtain plot should now auto update extent correctly in QGIS 3.20
          TUFLOW Viewer - Fixed bug when opening mesh layer properties with multiple results selected which would cause python error after selected a mesh layer
          TUFLOW Viewer - Animation tool will now correctly animate only the selected result in animation dialog
          TUFLOW Viewer - Fixed an error that could occur when saving default vector style while viewing netcdf results
          TUFLOW Viewer - FV netCDF results now correctly show dry areas when plotted
          Load From TCF - Rainfall control file now included
          Auto label - Fixed labelling tool so it correctly applies _messages.txt label properties to messages.shp
          1D Integrity Tool - Added label option to flow trace long section
          1D Integrity Tool - Fixed a bug that would result in an 'unexpected error'
          Import Empty - Added _pts to empty list
          ARR Tool - Fixed bug that would cause an error when adding additional temporal patterns due to areal temporal patterns not being downloaded correctly
          ARR Tool - Fixed bug that would not output 30m duration storm if 30h storm was also selected
          ARR Tool - Python version independent
          ARR Tool - Changed plotting backend to qt5agg
          Fixed bug that would cause TUFLOW plugin to not load if the netCDF4 Python library was not installed

          --- 3.1.8 ---
          SWAN GIS Tools - Added tool as beta to plugin
          TUFLOW Viewer - fixed bug that could occur when 'min_' was in the result type name that caused results to not load properly - usually resulting from outputs from res_to_res.exe
          TUFLOW Viewer - fixed bug that would cause Python error when exporting or copying plot data containing null x values and a datetime axis
          TUFLOW Viewer - Fixed bug that could cause 1D velocity TS to not plot if several results with different number of output times were selected
          TUFLOW Viewer - Added 'Redock TUFLOW Viewer' option under Settings menu in case TUFLOW Viewer gets stuck as a floating window and unable to dock
          TUFLOW Viewer - Export animation tool can once again automatically download ffmpeg.exe for Windows
          TUFLOW Viewer - Time slider will update properly when user switches between results (previously required user to change time to get it to update)
          TUFLOW Viewer - Updated the plot right-click context menu signal unloading to try and stop errors occuring when upgrading the plugin
          TUFLOW Viewer - Rename result functionality broke in QGIS 3.20 due to Python version upgrade
          ARR Tool - removed qt4agg backend dependency for plot generation - this could produce a warning message after running the tool
          TUFLOW Styling - Tweaked Flood Modeller result styling
          TUFLOW Styling - Added styling for lfcsh_uvpt_check

          --- 3.1.7 ---
          Auto Label - Added auto label rules for the _messages GIS layer
          TUFLOW Viewer - Fixed a bug that could occur when exporting plot to csv
          TUFLOW Viewer - Now catch issue when plot is empty when exporting or copying data - also added more messaging
          TUFLOW Viewer - Fixed a bug that could occur if more than 6 results were loaded at once that would cause TUFLOW Viewer to hang indefinitely
          TUFLOW Viewer - Fixed bug that would cause problems if mesh layer was renamed in QGIS layer panel
          TUFLOW Viewer - Fixed bug with map output cross-section plotting that could occur when output timesteps precision was finer than 1 second
          TUFLOW Viewer - Changed behaviour of plot when using 'show current time' - the vertical bar no longer affects plot extents and won't force plot to refresh
          TUFLOW Viewer - Unchecking legend position will also turn plot legend off
          ARR to TUFLOW - Updated routine that collects rainfall data from BOM
          ARR to TUFLOW - Added all column headers to output bc_dbase.csv

          --- 3.1.6 ---
          ARR tool - Fix bug that would not calculate burst initial loss correctly with user specified loss and probability neutral loss
          ARR tool - Probability neutral losses and complete storm check boxes are now mutually exclusive options in dialog
          Load TUFLOW Layers from TCF - MIF layers will automatically open all geometry types without user prompt
          Load TUFLOW Layers from TCF - Raster layers will be automatically be given the projection of first loaded vector layer if it doesn't have one
          TUFLOW Viewer - Fixed bug in 'Remove - Map Outputs' that would remove the layer from QGIS but not from TUFLOW Viewer
          TUFLOW Viewer - Load FM time series results will now create cross-sections based on gxy file if not already georeferenced
          TUFLOW Viewer - Load FM time series results corrected fixed field error in reading dat file that would cause incorrect unit names
          TUFLOW Viewer - Fixed vertical profile plotting when adding to an animation
          TUFLOW Viewer - Fixed a few bugs in batch map export tool, mainly fixes for latest QGIS API
          TUFLOW Viewer - Fixed dat file loading
          TUFLOW Viewer - Fixed TUFLOW FV xmdf loading
          TUFLOW Viewer - Narrow view will now remember last docked location (if set as default layout)
          TUFLOW Viewer - Fixed bug - first time results are loaded, the times are offset by user's time zone
          TUFLOW Viewer - Batch export plots will now remove any mesh results when finished plotting from them that were loaded by the tool
          TUFLOW Viewer - Plot right-click context menu will no longer appear if plot pan or zoom tools are in use
          TUFLOW Viewer - Re-organised 'Settings >> Options' dialog box in a new tab layout
          TUFLOW Viewer - Added legend font size option, axis font size option, axis label font size option
          TUFLOW Viewer - Added option to set a default plot font size
          TUFLOW Viewer - Fixed a bug that would cause python error when user selected 'Show as dates' when 'show current time' was on and secondary axis was also in use
          TUFLOW Viewer - Fixed bug that would cause python error if user 'cleared plot' while in the middle of drawing a plot location
          TUFLOW Viewer - Added user defined plot background colour (in settings >> options)
          TUFLOW Viewer - Added more customisable legend options (position, orientation)
          TUFLOW Viewer - Exporting drawn plot lines / points to shp is now exported to a 2d_po format
          TUFLOW Viewer - Fixed axis mis-naming when plotting flow regime (was incorrectly using flow units)
          TUFLOW Viewer - Fixed bug when trying to plot with dates after toggling on/off secondary axis
          TUFLOW Viewer - Fixed bug in User Plot Data Manager that would cause issues if user changed dataset name
          TUFLOW Viewer - Fixed bug that would only display User Plot Data on time series plot (regardless of selected 'plot type')
          TUFLOW Viewer - Fixed bug that would cause python error when trying to view user plot data in manager if selection was on the 'plot type'
          TUFLOW Viewer - Fixed bug when loading from TLF that would prevent load if there were periods in file name

          --- 3.1.5.5 ---
          TUFLOW Viewer - Added plot value display when plot is clicked

          --- 3.1.5.4 ---
          ARR tool - fixed ARF for catchments less than 10km2 that caused python error (introduced in 3.1.5)

          --- 3.1.5.3 ---
          TUFLOW Viewer - Fixed bug that would cause python error when changing 'zero date'
          TUFLOW Viewer - Fixed bug that would cause python error if 1D 'losses' plot option was selected with a 2D plot object selected
          TUFLOW Viewer - Fixed bug that would make mesh disappear when switching between results if "show grid" was on
          Import Empty Tool - Fixed bug that would cause error if overwriting existing file
          Import Empty Tool - Fixed typo in error message "No Empty File T specified" should be "No Empty File specified"

          --- 3.1.5 ---
          SCS Curve number calculation and export to TUFLOW tool added (beta)
          ReFH2 tool - ReFH2 engine 2.3 option added
          ReFH2 tool - Added climate change options
          ReFH2 tool - Added urban area input option
          ReFH2 tool - Added version and BFIHOST19 input check
          ReFH2 tool - Added engine version option
          ARR tool - NSW datahub continuing loss multiplied by 0.4
          ARR tool - let users set event independent continuing loss
          ARR tool - now recognises NaN rainfall loss values from the datahub and sets losses to zero
          ARR tool - Fixed bug that miscalculated ARF for short durations for catchments between 1 - 10km2
          TUFLOW Viewer - Import FM timeseries results added
          TUFLOW Viewer - Fixed bug that would incorrectly flag layers as 1D cross section and cause QGIS to hang
          TUFLOW Viewer - Customising plot 'select axes' dialog has nicer labels 'primary axis' and 'secondary axis'
          TUFLOW Viewer - Minimums fixed for TUFLOW Classic results when importing XMDF
          TUFLOW Viewer - Fixed a bug in animation tool that would error when adding plots if current time was already displayed in time series plot window
          TUFLOW Viewer - Fixed an issue with connection signals trying to persist after tuflow viewer is completely closed
          TUFLOW Viewer - Fixed vertical profile plotting - broke with new python version
          TUFLOW Viewer - For QGIS 3.16+ TUFLOW viewer now adopts absolute time as default (internal workings - no change for users)
          TUFLOW Utilities tool - Fixed the downloader - exe location was not being correctly input
          TUFLOW Utilities tool - Made further improvements to error checking
          Import check files tool - Fixed bug in import all check files from a folder where it would duplicate layers
          Reload layer tool -  no longer produces an error for non-vector layers - it still only works for vector layers
          Many small bug fixes

          --- 3.1.4.1 ---
          Uninstalling plugin should now work unless the ReFH2 tool has been run

          --- 3.1.4 ---
          Prj string for shp files are retained with increment and import empty tools
          Maximums in TUFLOWFV dat files now handled
          Fixed bug that would cause python error when saving project after updating colour ramp options for curtain plots
          Utility download links updated to reflect new website
          Fixed bug in ARR tool that would cause tool to crash when using probability neutral losses

          ---  3.1.3 ---
          Fixed 'Close TUFLOW Viewer completely
          Fixed bug in curtain plots with quadtree results
          Further plugin unloading improvements
          Fixed a few bugs in batch export
          Fixed bug where saving a project would stop user from being able to change zero time (tuflow classic)

          ---  3.1.2.3 ---
          Mulitple curtain plots (lines and result types) now supported - useful for animations

          ---  3.1.2.2 ---
          Batch export plot now supports selecting results not yet loaded into QGIS

          ---  3.1.2.1  ---
          Fixed bug when curtain plotting TUFLOW FV results
          Fixed datetime bug in animation tool

          ---  3.1.2  ---
          XS viewer will now load null or blank entries
          Depth time series added
          Added reset all plot colours to settings menu
          Fixed issue with unloading plugin
          Fixed qgs temporal controller interaction
          Fixed errors when saving and loading project settings
          Fixed bug when plotting flow from cell centred netcdf results
          Fixed bug for QGIS 3.14+ when using small output intervals
          Fixed a couple of errors with loading default styles
          Fixed bug in animation tool when adding a plot with a secondary axis
          Fixed issue when loading in time series results with '[' in run name
          TUFLOW styling will check style folder first before applying any defaults

          ---  3.1.1  ---
          Fixed backward compatibility

          ---  3.1.0  ---
          Compatible with QGIS temporal controller
          Added new plotting types for 3D datasets
          Added Cross section viewing capabilities
          Added ability to load 1D hydraulic check files
          Added particle tracking loading / viewing
          Added further error checking / messaging to 1D integrity tool
          Fixed bug in ARR tool that would occur when adding additional temporal patterns with large catchments that required Areal TP
          Fixed minor bug with case sensitivity when loading results through TCF file
          Removed message window "appended .shp to output" from increment tool

# tags are comma separated with spaces allowed
tags=TUFLOW, simulation, flood, hydraulic modelling, MDAL, mesh, xmdf, dat, 2dm, Australian Rainfall & Runoff, ARR, ReFH2

homepage=https://wiki.tuflow.com/index.php?title=TUFLOW_QGIS_Plugin
tracker=https://github.com/TUFLOW-Support/QGIS-TUFLOW-Plugin/issues
repository=https://github.com/TUFLOW-Support/QGIS-TUFLOW-Plugin
icon=tuflow.png
# experimental flag
experimental=False

# deprecated flag (applies to the whole plugin, not just a single version)
deprecated=False

