location == TUFLOW FV Control File (.fvc)

command == Read GIS PO

description == Used to define the 2D and 3D point plot output locations. If running a 3D model, for a given point location the vert_min and vert_max attributes will override the 
default vertical averaging limits (0,99999.) or those specified via the Vertical Averaging == output block command

See https://fvwiki.tuflow.com/Tutorial_M04 for example.


