This tool identifies the nodes snapped to the endpoints of conduits and assigns the "To Node" and "From Node" appropriately.

This tool supports in-place editing if selected in the QGIS processing window.