location == ESTRY Control File (.ecf)

command == Read GIS Table Links

description == Reads links to tabular inputs associated with cross-section profiles (1d_xs), nodal surface areas (1d_na) and bridge loss coefficients (1d_bg).

wiki link == https://wiki.tuflow.com/TUFLOW_Empty_Files#ESTRY_Control_file_.28ECF.29

manual link == https://www.tuflow.com/Download/TUFLOW/Releases/2017-09/TUFLOW%20Manual.2017-09-AC.pdf
manual page == 90