location == TUFLOW Control File (.tcf)

command == Read GIS GLO

description == Used to define gauge level output (2d_glo) locations. The GLO command controls map output based on the height of the water at a specified location within the model domain.

wiki link == https://wiki.tuflow.com/index.php?title=TUFLOW_Empty_Files#TUFLOW_Control_file_.28TCF.29

manual link == https://downloads.tuflow.com/_archive/TUFLOW/Releases/2018-03/TUFLOW%20Manual.2018-03.pdf
manual page == 391