In some applications it is necessary to relate a measured variable for a group of hydrometric stations (e.g. characteristics of flow timing and duration or water chemistry) to some characteristics of each outlet's catchment (e.g. mean slope, area of wetlands, etc.). When the group of outlets are nested, i.e. some stations are located downstream of others, then performing a watershed operation will result in inappropriate watershed delineation. In particular, the delineated watersheds of each nested outlet will not include the catchment areas of upstream outlets. This creates a serious problem for this type of application.

The Unnest Basin tool can be used to perform a watershedding operation based on a group of specified pour points, i.e. outlets or target cells, such that each complete watershed is delineated. The user must specify the name of a flow pointer (flow direction) raster, a pour point raster, and the name of the output rasters. Multiple numbered outputs will be created, one for each nesting level. Pour point, or target, cells are denoted in the input pour-point image as any non-zero, non-NoData value. The flow pointer raster should be generated using the D8 algorithm.

## Function Signature

`def unnest_basins(self, d8_pointer: Raster, pour_points: Vector, esri_pntr: bool = False) -> List[Raster]: ...`

## Project Links

WbW Homepage User Manual Support WbW