This tool can be used to measure the slope gradient, in degrees, each grid cell in a raster stream network. To estimate the average slope for each link in a stream network, use the stream_link_slope tool instead. The user must input a stream raster image (`streams_raster`), a D8 pointer image (d8_pointer), and a digital elevation model (`dem`). The pointer image is used to traverse the stream network and must only be created using the D8 algorithm (d8_pointer). Stream cells are designated in the streams image as all values greater than zero. Thus, all non-stream or background grid cells are commonly assigned either zeros or NoData values. Background cells will be assigned the NoData value in the output image, unless `zero_background=True`, in which case non-stream cells will be assigned zero values in the output.

By default, the pointer raster is assumed to use the clockwise indexing method used by WhiteboxTools. If the pointer file contains ESRI flow direction values instead, set `esri_pointer=True`.

## See Also

stream_link_slope, d8_pointer

## Function Signature

`def stream_slope_continuous(self, d8_pointer: Raster, streams_raster: Raster, dem: Raster, esri_pointer: bool = False, zero_background: bool = False) -> Raster: ...`

## Project Links

WbW Homepage User Manual Support WbW