This tool can be used to plot a histogram of data derived from a LiDAR file. The user must specify the name of the input LAS file (`input`), the name of the output HTML file (`output`), the parameter (`parameter`) to be plotted, and the amount (in percent) to clip the upper and lower tails of the f requency distribution (clip). The LiDAR parameters that can be plotted using lidar_histogram include the point elevations, intensity values, scan angles, and class values.

Use the lidar_point_stats tool instead to examine the spatial distribution of LiDAR points.

## See Also

lidar_point_stats

## Function Signature

`def lidar_histogram(self, input_lidar: Lidar, output_html_file: str, parameter: str = "elevation", clip_percent: float = 1.0) -> None: ...`

## Project Links

WbW Homepage User Manual Support WbW