# SAGA Wetness Index

(c) 2001 by J.Boehner, O.Conrad
The 'SAGA Wetness Index' is, as the name says, similar to the 'Topographic Wetness Index' (TWI), but it is based on a modified catchment area calculation ('Modified Catchment Area'), which does not think of the flow as very thin film. As result it predicts for cells situated in valley floors with a small vertical distance to a channel a more realistic, higher potential soil moisture compared to the standard TWI calculation.
References
- Boehner, J., Koethe, R. Conrad, O., Gross, J., Ringeler, A., Selige, T. (2002): Soil Regionalisation by Means of Terrain Analysis and Process Parameterisation. In: Micheli, E., Nachtergaele, F., Montanarella, L. [Ed.]: Soil Classification 2001. European Soil Bureau, Research Report No. 7, EUR 20398 EN, Luxembourg. pp.213-222.

## Parameters

Grid system
Grid system
  Grid system
Elevation
Input Grid
Catchment area
Output Grid
Catchment slope
Output Grid
Modified catchment area
Output Grid
Wetness index
Output Grid
t
Floating point