# Convert Data Storage Type

O.Conrad (c) 2003
Changes the storage data type of a grid (e.g. from 4 byte floating point to 2 byte signed integer). If the target is not set, the original grid's storage type will be changed.

## Parameters

Grid system
Grid system
  Grid system
Grid
Input Grid
Converted Grid
Output Grid
Data storage type
Choice
  Available choices: bit, unsigned 1 byte integer, signed 1 byte integer, unsigned 2 byte integer, signed 2 byte integer, unsigned 4 byte integer, signed 4 byte integer, 4 byte floating point number, 8 byte floating point number