[general]
name=AGLgis
qgisMinimumVersion=3.28
qgisMaximumVersion=4.99
description=Sentinel-1 SAR (VV/VH) backscatter time series and analysis-ready data preparation in Google Earth Engine — cloud-independent / Séries temporais de retroespalhamento SAR Sentinel-1 (VV/VH) e preparo de dados no Google Earth Engine — independente de nuvens
version=9.2
author=FARM Analytica
email=contato@farmanalytica.com.br

about=AGLgis is a graphical interface for Sentinel-1 SAR Backscatter Analysis-Ready-Data preparation in Google Earth Engine, inside QGIS. Build VV/VH backscatter time series for cloud-independent monitoring of crops, water and land surfaces, with border-noise correction, terrain flattening and speckle filtering. Requires a Google Earth Engine account (sign-in and a project ID are set up inside the plugin). / O AGLgis é uma interface gráfica para o preparo de dados de retroespalhamento SAR Sentinel-1 (Analysis-Ready Data) no Google Earth Engine, dentro do QGIS. Gere séries temporais VV/VH para monitoramento independente de nuvens de culturas, água e superfícies, com correção de ruído de borda, achatamento de terreno e filtragem de speckle. Requer uma conta do Google Earth Engine (login e ID de projeto são configurados dentro do plugin).

tracker=https://github.com/farmanalytica/farm_tools/issues
repository=https://github.com/farmanalytica/farm_tools
# End of mandatory metadata

# Recommended items:

hasProcessingProvider=no
changelog=
    9.0 - RAVI plot date-range filtering: two-handle slider below the plot lets
          you narrow the cached time series by date span. Dragging updates the
          label live and re-renders the plot after settling (200 ms debounce).
          The date selection ANDs with existing filters (thresholds, manual
          per-date selection) and automatically constrains composite generation,
          batch download, CSV export, and single-image dropdown. RangeSlider
          widget gains optional label_fn for custom value→text mapping (e.g.
          day offsets to ISO dates), adaptive label width, and set_span()
          reconfig without signal emission. Numeric year-range path (MapBiomas
          transition, SYSI filters) untouched. AOI-area label on Inputs tab
          shows hectares below the layer picker. Management Zones module:
          integrated fork of Precision Zones for defining and analyzing
          management boundaries within fields, with zoning workflows, per-zone
          statistics, and export to QGIS for further analysis. Zone outputs
          save to the global download folder from the Welcome page (per-module
          folder picker removed). Data tab UX: the input-raster list stays in
          sync with the project (add/remove/rename), rasters are picked with
          checkboxes, and resolution defaults to 10 m. Generate zones can
          optionally apply the mode (majority) filter to the output in one
          step, and generated/filtered zone rasters load with a single-band
          pseudocolor renderer and a selectable color ramp. Resampling and the
          elbow + silhouette analysis run in background workers: the dialog
          stays responsive, buttons show live progress, and a second click
          cancels the run. Silhouette scores are subsampled on large grids for
          much faster cluster evaluation.
    8.0 - now built from the unified FARM tools codebase. Ships defaulting to this module; the other FARM tools modules are discoverable from the welcome page's "More tools" section and as separate plugins.

# Tags are comma separated with spaces allowed
tags=python, sentinel, sentinel-1, radar, sar, backscatter, google earth engine, remote sensing, raster, agriculture

homepage=https://farmtools.org
category=Raster
icon=icon.png
experimental=False
deprecated=False
server=False
