# GeoDyn for municipalities with support for GWSW standard

DISCLAIMER: this plugin is still in development!

GeoDynGemeentenGWSW is developed by BKGIS and Jafeth Heining and designed by Mark Lamers.

Tool for calculating wastewater prognosis based on
- Municipal sewage systems (Kikker riodesk and GWSW) 
- Residental data (BAG)
- Housing development plans RIGO (https://www.plancapaciteit.nl/)
- Household drinking water consumption

This tool is based on GeoDynWaterschap. GeoDynWaterschap is an ArcGIS 10
toolbox for the Dutch Water Authorities. GeoDynWaterschap is develop by BKGIS, for
the water Authority HHNK and designed by Mark Lamers.

# Manual
https://github.com/bart147/GeoDynGemGWSW/blob/master/doc/HandleidingGeoDynGemGWSW.pdf

# Installation
- Install the plugin with Plugin Manager in QGIS or download here https://plugins.qgis.org/plugins/GeoDynGemGWSW/
- Requires QGIS 3.16 or higher

# Test data
Some imaginary data for testing can be downloaded from the repo:
https://github.com/bart147/GeoDynGemGWSW/blob/master/input_test_gpkg


