[general]
name=QDebrisFlow
qgisMinimumVersion=3.16
description=Modelling of post-fire debris flows (O'Brien quadratic rheology + LIA). Individual source hydrographs, 5-tab interface, output layer selection, LHS analysis.
version=1.0
author=Aidar Khaybulin, Anna Zatonskaya, Alexander Panchenko
email=batmeny@gmail.com
about=Models post-fire debris flows based on the quadratic rheological model of O'Brien and Julien (1985, 1988) and the local inertial approximation of the shallow water equations (LIA). Based on the FLO-2D formulation. Outputs: maximum depth envelope (h_max), maximum velocity (V_max), final deposit (h_final), flow arrival time map.
tracker=https://github.com/Oidorrr/QDebrisFlow/issues
repository=https://github.com/Oidorrr/QDebrisFlow
tags=debris flow,mudflow,hazard,rheology,post-fire
homepage=https://github.com/Oidorrr/QDebrisFlow
category=Raster
icon=icon.png
experimental=True
deprecated=False
