### Navigation

- index
- modules
- Home »
- Contents »
- Module code »

# Source code for safe.impact_functions.earthquake.itb_earthquake_fatality_model

    from safe.impact_functions.core import FunctionProvider
    from safe.impact_functions.core import get_hazard_layer, get_exposure_layer
    from safe.impact_functions.core import get_question
    from safe.storage.raster import Raster
    from safe.common.utilities import ugettext as tr
    from safe.common.tables import Table, TableRow
    from safe.common.exceptions import InaSAFEError

    import numpy

    class ITBFatalityFunction(FunctionProvider):
        """Indonesian Earthquake Fatality Model

        This model was developed by Institut Tecknologi Bandung (ITB) and
        implemented by Dr Hadi Ghasemi, Geoscience Australia

        Reference:

        Indonesian Earthquake Building-Damage and Fatality Models and
        Post Disaster Survey Guidelines Development,
        Bali, 27-28 February 2012, 54pp.

        Algorithm:

        In this study, the same functional form as Allen (2009) is adopted
        to express fatality rate as a function of intensity (see Eq. 10 in the
        report). The Matlab built-in function (fminsearch) for  Nelder-Mead
        algorithm is used to estimate the model parameters. The objective
        function (L2G norm) that is minimised during the optimisation is the
        same as the one used by Jaiswal et al. (2010).

        The coefficients used in the indonesian model are
        x=0.62275231, y=8.03314466, zeta=2.15

        Allen, T. I., Wald, D. J., Earle, P. S., Marano, K. D., Hotovec, A. J.,
        Lin, K., and Hearne, M., 2009. An Atlas of ShakeMaps and population
        exposure catalog for earthquake loss modeling, Bull. Earthq. Eng. 7,
        701-718.

        Jaiswal, K., and Wald, D., 2010. An empirical model for global earthquake
        fatality estimation, Earthq. Spectra 26, 1017-1037.

        Caveats and limitations:

        The current model is the result of the above mentioned workshop and
        reflects the best available information. However, the current model
        has a number of issues listed below and is expected to evolve further
        over time.

        1 - The model is based on limited number of observed fatality
            rates during 4 past fatal events.
        2 - The model clearly over-predicts the fatality rates at
            intensities higher than VIII.
        3 - The model only estimates the expected fatality rate for a given
            intensity level; however the associated uncertainty for the proposed
            model is not addressed.
        4 - There are few known mistakes in developing the current model:
            - rounding MMI values to the nearest 0.5,
            - Implementing Finite-Fault models of candidate events, and
            - consistency between selected GMPEs with those in use by BMKG.
              These issues will be addressed by ITB team in the final report.

        :author Hadi Ghasemi
        :rating 3

        :param requires category=='hazard' and \
                        subcategory=='earthquake' and \
                        layertype=='raster' and \
                        unit=='MMI'

        :param requires category=='exposure' and \
                        subcategory=='population' and \
                        layertype=='raster'

        """

        parameters = dict(x=0.62275231, y=8.03314466,  # Model coefficients
                          # Rates of people displaced for each MMI level
                          displacement_rate={1: 0, 2: 0, 3: 0, 4: 0, 5: 0, 6: 1.0,
                                             7: 1.0, 8: 1.0, 9: 1.0, 10: 1.0},
                          # Threshold below which layer should be transparent
                          tolerance=0.01,
                          calculate_displaced_people=True)
        title = tr('Die or be displaced')

        def run(self, layers):
            """Indonesian Earthquake Fatality Model

            Input
              layers: List of layers expected to contain
                  H: Raster layer of MMI ground shaking
                  P: Raster layer of population density

            """

            # Establish model coefficients
            x = self.parameters['x']
            y = self.parameters['y']

            # Define percentages of people being displaced at each mmi level
            displacement_rate = self.parameters['displacement_rate']

            # Tolerance for transparency
            tolerance = self.parameters['tolerance']

            # Extract input layers
            intensity = get_hazard_layer(layers)
            population = get_exposure_layer(layers)

            question = get_question(intensity.get_name(),
                                    population.get_name(),
                                    self)

            # Extract data grids
            H = intensity.get_data()   # Ground Shaking
            P = population.get_data(scaling=True)  # Population Density

            # Calculate population affected by each MMI level
            # FIXME (Ole): this range is 2-9. Should 10 be included?
            mmi_range = range(2, 10)
            number_of_exposed = {}
            number_of_displaced = {}
            number_of_fatalities = {}

            # Calculate fatality rates for observed Intensity values (H
            # based on ITB power model
            R = numpy.zeros(H.shape)
            for mmi in mmi_range:

                # Identify cells where MMI is in class i
                mask = (H > mmi - 0.5) * (H <= mmi + 0.5)

                # Count population affected by this shake level
                I = numpy.where(mask, P, 0)

                # Calculate expected number of fatalities per level
                fatality_rate = numpy.power(10.0, x * mmi - y)
                F = fatality_rate * I

                # Calculate expected number of displaced people per level
                try:
                    D = displacement_rate[mmi] * I
                except KeyError, e:
                    msg = 'mmi = %i, I = %s, Error msg: %s' % (mmi, str(I), str(e))
                    raise InaSAFEError(msg)

                # Adjust displaced people to disregard fatalities.
                # Set to zero if there are more fatalities than displaced.
                D = numpy.where(D > F, D - F, 0)

                # Sum up numbers for map
                R += D   # Displaced

                # Generate text with result for this study
                # This is what is used in the real time system exposure table
                number_of_exposed[mmi] = numpy.nansum(I.flat)
                number_of_displaced[mmi] = numpy.nansum(D.flat)
                number_of_fatalities[mmi] = numpy.nansum(F.flat)

            # Set resulting layer to NaN when less than a threshold. This is to
            # achieve transparency (see issue #126).
            R[R < tolerance] = numpy.nan

            # Total statistics
            total = int(round(numpy.nansum(P.flat) / 1000) * 1000)

            # Compute number of fatalities
            fatalities = int(round(numpy.nansum(number_of_fatalities.values())
                                   / 1000)) * 1000

            # Compute number of people displaced due to building collapse
            displaced = int(round(numpy.nansum(number_of_displaced.values())
                                  / 1000)) * 1000

            # Generate impact report
            table_body = [question]

            # Add total fatality estimate
            s = str(int(fatalities)).rjust(10)
            table_body.append(TableRow([tr('Number of fatalities'), s],
                                       header=True))

            if self.parameters['calculate_displaced_people']:
                # Add total estimate of people displaced
                s = str(int(displaced)).rjust(10)
                table_body.append(TableRow([tr('Number of people displaced'), s],
                                           header=True))
            else:
                displaced = 0

            # Add estimate of total population in area
            s = str(int(total)).rjust(10)
            table_body.append(TableRow([tr('Total number of people'), s],
                                       header=True))

            # Calculate estimated needs based on BNPB Perka 7/2008 minimum bantuan
            rice = displaced * 2.8
            drinking_water = displaced * 17.5
            water = displaced * 67
            family_kits = displaced / 5
            toilets = displaced / 20

            # Generate impact report for the pdf map
            table_body = [question,
                          TableRow([tr('Fatalities'),
                                    '%i' % fatalities],
                                   header=True),
                          TableRow([tr('People displaced'),
                                    '%i' % displaced],
                                   header=True),
                          TableRow(tr('Map shows density estimate of '
                                      'displaced population')),
                          TableRow([tr('Needs per week'), tr('Total')],
                                   header=True),
                          [tr('Rice [kg]'), int(rice)],
                          [tr('Drinking Water [l]'), int(drinking_water)],
                          [tr('Clean Water [l]'), int(water)],
                          [tr('Family Kits'), int(family_kits)],
                          [tr('Toilets'), int(toilets)]]
            impact_table = Table(table_body).toNewlineFreeString()

            table_body.append(TableRow(tr('Action Checklist:'), header=True))
            if fatalities > 0:
                table_body.append(tr('Are there enough victim identification '
                                     'units available for %i people?') %
                                     fatalities)
            if displaced > 0:
                table_body.append(tr('Are there enough shelters and relief items '
                                     'available for %i people?') % displaced)
                table_body.append(TableRow(tr('If yes, where are they located and '
                                              'how will we distribute them?')))
                table_body.append(TableRow(tr('If no, where can we obtain '
                                              'additional relief items from and '
                                              'how will we transport them?')))

            # Extend impact report for on-screen display
            table_body.extend([TableRow(tr('Notes'), header=True),
                               tr('Total population: %i') % total,
                               tr('People are considered to be displaced if '
                                  'they experience and survive a shake level'
                                  'of more than 5 on the MMI scale '),
                               tr('Minimum needs are defined in BNPB '
                                 'regulation 7/2008')])

            impact_summary = Table(table_body).toNewlineFreeString()
            map_title = tr('People in need of evacuation')

            table_body.append(TableRow(tr('Notes'), header=True))
            table_body.append(tr('Fatality model is from '
                                'Institute of Teknologi Bandung 2012.'))
            table_body.append(tr('Population numbers rounded to nearest 1000.'))

            impact_summary = Table(table_body).toNewlineFreeString()
            impact_table = impact_summary
            map_title = tr('Earthquake impact to population')

            # Create style info dynamically
            classes = numpy.linspace(numpy.nanmin(R.flat[:]),
                                     numpy.nanmax(R.flat[:]), 5)

            style_classes = [dict(colour='#EEFFEE', quantity=classes[0],
                                  transparency=100,
                                  label=tr('%.2f people/cell') % classes[0]),
                             dict(colour='#FFFF7F', quantity=classes[1],
                                  transparency=30),
                             dict(colour='#E15500', quantity=classes[2],
                                  transparency=30,
                                  label=tr('%.2f people/cell') % classes[2]),
                             dict(colour='#E4001B', quantity=classes[3],
                                  transparency=30),
                             dict(colour='#730000', quantity=classes[4],
                                  transparency=30,
                                  label=tr('%.2f people/cell') % classes[4])]
            style_info = dict(target_field=None,
                              style_classes=style_classes)

            # Create new layer and return
            L = Raster(R,
                       projection=population.get_projection(),
                       geotransform=population.get_geotransform(),
                       keywords={'impact_summary': impact_summary,
                                 'total_population': total,
                                 'total_fatalities': fatalities,
                                 'impact_table': impact_table,
                                 'map_title': map_title},
                       name=tr('Estimated displaced population'),
                       style_info=style_info)

            # Maybe return a shape file with contours instead
            return L

### Navigation

- index
- modules
- Home »
- Contents »
- Module code »