### Add tag to selected waypoints

After selecting a waypoint or multiple waypoints (see FAQ) and pressing this button, a label is added to the point.

You can choose from the following predefined tags:

- FLYOVER
- FLYBY
- RH180 – Right Hand 180°
- RH270 – Right Hand 270°
- LH180 – Left Hand 180°
- LH270 – Left Hand 270°

Additionally, you can create a custom tag. Please ensure that the custom tag adheres to the following restrictions; otherwise, it will not be added.

Restrictions for custom tags:

- May only consist of capital letters (upper case), whitespaces, and the backslash (/) character.
- Must not exceed 10 characters.

Viewing Tags:

After adding a tag, select the corresponding waypoint to see the tag displayed in the status bar at the bottom of the screen.

To view all waypoints and their associated tags:

1. Select the waypoint layer.
2. Open the Attribute Table (right-click → “Open Attribute Table”).