[general]
name=Sen Couverture Terrestre
qgisMinimumVersion=3.16
description=Per-commune analysis for Senegal: Sentinel-2 land cover (Living Atlas), soil type and estimated fertility (Morpho_Pedo), and relief (DEM).
version=1.2.1
author=ADIOUMA FALL -Géo
email=mouridefalltouba@gmail.com

about=This plugin lets you pick a commune (municipality) in Senegal, zoom to it automatically, download and clip Sentinel-2 10m land cover (ArcGIS Living Atlas, 2017-2024) to its exact boundary, and display soil type statistics (estimated fertility) and relief statistics from reference layers bundled with the plugin (communes and pedology, no manual import needed). Relief includes min/max/mean altitude, elevation range, mean/min/max slope, and FAO slope-class breakdown. The DEM can be selected as an external file, processed entirely in the background and never added to the layers panel.
 French description: Ce plugin permet de selectionner une commune du Senegal, de zoomer automatiquement dessus, de telecharger et decouper la couverture terrestre Sentinel-2 10m (ArcGIS Living Atlas, 2017-2024) sur sa limite exacte, et d'afficher des statistiques de type de sol (fertilite estimee) et de relief a partir des couches de reference integrees au plugin (communes et pedologie embarquees, aucun import manuel necessaire). Le relief inclut l'altitude min/max/moyenne, le denivele, la pente moyenne/min/max et sa repartition par classes FAO. Le MNT peut etre selectionne en fichier exterieur, traite entierement en arriere-plan sans jamais etre ajoute au panneau des couches.

changelog=1.2.1 (2026-07-23)
 - Fix: security scan issues (B310 URL scheme validation on ArcGIS export calls, B110 silent except/pass replaced with logged warning)
 1.2.0 (2026-07-23)
 - Add: elevation range (max-min) and min/max slope in addition to the mean
 - Add: FAO slope-class breakdown (Flat/Gentle/Moderate/Steep/Very steep)
 - Add: bundled reference layers (communes, soil type), loaded automatically
 - Add: remembered DEM file selection, processed in the background without adding it to the layers panel
 - Fix: commune name field detection (CCRCA) and default soil layer
 - Fix: wrong slope-class areas on a geographic-CRS DEM (added EPSG:32628 reprojection)

tracker=https://github.com/Ghostline1313/sen_couverture_terrestre/issues
repository=https://github.com/Ghostline1313/sen_couverture_terrestre
tags=arcgis,living atlas,esri,sol,pedologie,fertilite,relief,rest api,senegal,sen hydro
homepage=https://github.com/Ghostline1313/sen_couverture_terrestre
category=Web
license=GPL-3.0-or-later
icon=icon.png
experimental=False
deprecated=False
server=False
hasProcessingProvider=no

