TPI Based Landform Classification
ta_morphometry
ParameterRaster|DEM|Elevation|False
ParameterNumber|RADIUS_A_MIN|Min Radius A|None|None|0
ParameterNumber|RADIUS_A_MAX|Max Radius A|None|None|100
ParameterNumber|RADIUS_B_MIN|Min Radius B|None|None|0
ParameterNumber|RADIUS_B_MAX|Min Radius B|None|None|1000
ParameterSelection|DISTANCE_WEIGHTING_WEIGHTING|Distance Weighting|[0] no distance weighting;[1] inverse distance to a power;[2] exponential;[3] gaussian weighting
ParameterNumber|DISTANCE_WEIGHTING_IDW_POWER|Inverse Distance Weighting Power|0.0|None|1
ParameterBoolean|DISTANCE_WEIGHTING_IDW_OFFSET     |Inverse Distance Offset|True
ParameterNumber|DISTANCE_WEIGHTING_BANDWIDTH|Gaussian and Exponential Weighting Bandwidth|None|None|75.0
OutputRaster|LANDFORMS|Landforms
