How would you like to process the input DEM:
Choose the processing tool you want to use.

This tool allows you to copy elevation values from a raster into another one. The elevation values of the pixels covered by a mask will be copied into the second raster.

Please note that the area you copy from the original raster will be in the same position in the target raster.

Raster to be modified:
Choose the DEM you want to copy the elevation values to.

Raster to copy the values from:
Choose the DEM you want to copy the values from.

Mask layer:
Select the vector layer containing the masks covering the areas you want to copy.

If you want to use only certain masks of the mask layer, you can select these masks on the map canvas and then check the Selected features only checkbox.

Output file path:
If there is no path specified here, the file will be created in the temporary folder. The full path will be shown in the Log tab and the result will be loaded to the map canvas.

Warning: Please avoid using these characters in the file name, as they might cause processing errors: ( ) / - % $ @ #
Note: If this tool is used repetitively with no path specified, previous results will be overwritten. To avoid this, specify a different path (or filename) each time