location == Geometry Control File (.tgc)

command == Read GIS CWF

description == Used to adjust the 2D cell flow widths. The CWF is a factor, for example 0.1 will limit the flow width to 10%. The changed flow width applies to all depths. 

wiki link == https://wiki.tuflow.com/TUFLOW_Empty_Files#TUFLOW_Geometry_Control_file_.28TGC.29

manual link == https://docs.tuflow.com/classic-hpc/manual/2026.0/TwoD-Domains-1.html#CWF-4