## License Information

Use of this function requires a license for Whitebox Workflows for Python Professional (WbW-Pro). Please visit www.whiteboxgeo.com to purchase a license.

## Description

This tool can be used to fix undershot and overshot arcs, two common topological errors, in an input vector lines file (`input`). In addition to the input lines vector, the user must also specify the output vector (`output`) and the snap distance (`snap`). All dangling arcs that are within this threshold snap distance of another line feature will be connected to the neighbouring feature. If the input lines network is a vector stream network, users are advised to apply the repair_stream_vector_topology tool instead.

## See Also

repair_stream_vector_topology, clean_vector

## Project Links

WbW Homepage User Manual Support WbW