Experimental

Snaps nearby polyline endpoints to a shared location within a tolerance.

vector gis linework legacy-port

## Parameters

Name | Description | Required | Default
--- | --- | --- | ---
`input` | Input polyline vector layer. | Required | `input_lines.shp`
`snap_tolerance` | Endpoint snapping tolerance in map units. | Optional | `2.220446049250313e-16`
`output` | Output snapped polyline vector path. | Required | —

## Examples

Snaps adjacent line endpoints by a tolerance threshold.

    wbe.snap_endnodes(input='input_lines.shp', output='snapped_endnodes.shp', snap_tolerance=2.220446049250313e-16)

## Project Links

WbW Homepage User Manual Support WbW