PRO Experimental

Locates low pass points along divides between neighboring headwater subbasins.

geomorphometry streams subbasins passes legacy-port

## Parameters

Name | Description | Required | Default
--- | --- | --- | ---
`dem` | Input depressionless DEM raster path or typed raster object. | Required | `dem.tif`
`streams` | Input stream raster path (positive values indicate channel cells). | Required | `streams.tif`
`output` | Optional output vector path (default temporary .shp). | Optional | `low_points_on_headwater_divides.shp`

## Examples

Find low pass points between neighboring headwater basins.

    wbe.low_points_on_headwater_divides(dem='dem.tif', output='low_points_on_headwater_divides.shp', streams='streams.tif')

## Project Links

WbW Homepage User Manual Support WbW